{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":11,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M"]
[]
[]
[]
[]
["","","","","","2AMXM40M3V1B","2AMXM40M4V1B","2AMXM40M2V1B","2AMXM50M2V1B","2AMXM50M4V1B","2AMXM50M3V1B"]
["Ventilator","Luftstromvolumen","Kühlung","Sehr niedrig","m³/min","","","30","34"]
["","","Heizen","Sehr niedrig","m³/min","","","32","34"]
["Schallleistungspegel","Heizen","","","dBA","","62","","","62"]
["","Kühlung","","","dBA","","60","","","60"]
["Ventilator","Luftstromvolumen","Kühlung","Sehr niedrig","cfm","","","1059","1200"]
["","","Heizen","Sehr niedrig","cfm","","","1130","1200"]
["Abmessungen","Maßeinheit","","Höhe","mm","550","550","550","550","550","550"]
["","","","Breite","mm","765","765","765","765","765","765"]
["","","","Tiefe","mm","285","285","285","285","285","285"]
["Gewicht","Maßeinheit","","","kg","36","36","36","41","41","41"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","500","500","760","890","500","500"]
["","","Heizen","Sehr niedrig","U/min","320","320","820","890","500","500"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","","46.0","-10","-10","46.0"]
["","","","Max.","°C TK","","-10","46","46","-10"]
["","Heizen","Umgebung","Min.","°C Feuchtkugel","","-15","","-15","-15.0"]
["","","","Max.","°C Feuchtkugel","","18.0","","18","18.0"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","46","46","","","48","48"]
["","","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dBA","","","","46"]
["","Heizen","","Hoch","dBA","48","48","","","50","50"]
["","","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dBA","","","","48"]
["Kältemittel","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Füllmenge","","","kg","0.88","0.88","0.88","1.15","1.15","1.15"]
["","Füllmenge","","","tCO2Eq","0.59","0.6","","0.8","0.78","0.78"]
["","GWP","","","","675.0","675","675","675","675","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","20","20 (1)","20","20","20 (1)","20"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 20 m)","0,02 (für Rohrleitungslängen über 20 m)","002 (für Rohrleitungslängen über 20 m)","0,02 (für Rohrleitungslängen über 20 m)","0,02 (für Rohrleitungslängen über 20 m)","0,02 (für Rohrleitungslängen über 20 m)"]
["","Niveauunterschied","IG - AG","Max.","M","15.0","15","15","15","15","15.0"]
["","","IG - IG","Max.","M","7.5","7.5","7.5","7.5","7.5","7.5"]
["","Gesamtleitungslänge","System","Ist","M","30","30","30","30","30","30"]
["Standardzubehör","Installation manual","","","","1","1","Installation manual","1","1","1"]
["","Drain plug","","","","1","1","Drain plug","1","1","1"]
["","Screw bag","","","","1","1","Screw bag","1","1","1"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-230-240","220-230-240","220-240","220-240","220-230-240","220-230-240"]
["Hinweise","","","","","(1) - Für 1 Raum","","(1) - Enthält fluorierte Treibhausgase","","","(1) - Für 1 Raum"]
["","","","","","","(1) - Für 1 Raum","","","(1) - Für 1 Raum"]
["","","","","","","(2) - Siehe separate Zeichnung für den Betriebsbereich","","","(2) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten","","","(3) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","","","(4) - Enthält fluorierte Treibhausgase","","","(4) - Enthält fluorierte Treibhausgase"]
["Verdichter","Typ","","","","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Heizen","Umgebung","Betriebsbereich-=-Heizen-=-Umgebung-=-Min.-=-°C FK","°C FK","","","-15"]
["","","","Betriebsbereich-=-Heizen-=-Umgebung-=-Max.-=-°C FK","°C FK","","","18"]
["Schalldruckpegel","Kühlung","","Nom.","dB(A)","","","48"]
["","Heizen","","Nom.","dB(A)","","","50"]
["Kältemittel","Kältemittel-=-Füllmenge-=-tCO2-Äq.","","","tCO2-Äq.","","","0.6"]
["Standardzubehör","Reducer assembly","","","","","","","1","1","1"]