{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M"]
[]
[]
[]
[]
["","","","","","2AMXM40M2V1B","2AMXM40M3V1B","2AMXM40M4V1B","2AMXM50M2V1B","2AMXM50M4V1B","2AMXM50M3V1B"]
["Ventilator","Luftstromvolumen","Kühlung","Sehr niedrig","m³/min","30","","","34"]
["","","Heizen","Sehr niedrig","m³/min","32","","","34"]
["Schallleistungspegel","Heizen","","","dB(A)","","","62","","62"]
["","Kühlung","","","dB(A)","","","60","","60"]
["Ventilator","Luftstromvolumen","Kühlung","Sehr niedrig","cfm","1059","","","1200"]
["","","Heizen","Sehr niedrig","cfm","1130","","","1200"]
["Abmessungen","Maßeinheit","","Höhe","mm","550","550","550","550","550","550"]
["","","","Breite","mm","765","765","765","765","765","765"]
["","","","Tiefe","mm","285","285","285","285","285","285"]
["Gewicht","Maßeinheit","","","kg","36","36","36","41","41","41"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","760","500","500","890","500","500"]
["","","Heizen","Sehr niedrig","U/min","820","320","320","890","500","500"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°CTK","-10","","46.0","-10","46.0"]
["","","","Max.","°CTK","46","","-10","46","-10"]
["","Heizen","Umgebung","Min.","°C FK","-15","","-15","-15","-15.0"]
["","","","Max.","°C FK","18","","18.0","18","18.0"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","","46","46","","48","48"]
["","","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dB(A)","48","","","46"]
["","Heizen","","Hoch","dB(A)","","48","48","","50","50"]
["","","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dB(A)","50","","","48"]
["Kältemittel","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Füllmenge","","","kg","0.88","0.88","0.88","1.15","1.15","1.15"]
["","Füllmenge","","","tCO2Eq","0.6","0.59","0.6","0.8","0.78","0.78"]
["","GWP","","","","675","675.0","675","675","675","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","20","20","20 (1)","20","20 (1)","20"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 20 m)","0,02 (für Rohrleitungslängen über 20 m)","0,02 (für Rohrleitungslängen über 20 m)","0,02 (für Rohrleitungslängen über 20 m)","0,02 (für Rohrleitungslängen über 20 m)","0,02 (für Rohrleitungslängen über 20 m)"]
["","Niveauunterschied","IG - AG","Max.","m","15","15.0","15","15","15","15.0"]
["","","IG - IG","Max.","m","7.5","7.5","7.5","7.5","7.5","7.5"]
["","Gesamtleitungslänge","System","Ist","m","30","30","30","30","30","30"]
["Standardzubehör","Installation manual","","","","Installation manual","1","1","1","1","1"]
["","Drain plug","","","","Drain plug","1","1","1","1","1"]
["","Screw bag","","","","Screw bag","1","1","1","1","1"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-230-240","220-230-240","220-240","220-230-240","220-230-240"]
["Hinweise","","","","","","(1) - Für 1 Raum","","","","(1) - Für 1 Raum"]
["","","","","","","","(1) - Für 1 Raum","","(1) - Für 1 Raum"]
["","","","","","","","(2) - Siehe separate Zeichnung für den Betriebsbereich","","(2) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten","","(3) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","","","","(4) - Enthält fluorierte Treibhausgase","","(4) - Enthält fluorierte Treibhausgase"]
["Standardzubehör","Reducer assembly","","","","","","","1","1","1"]