{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXF-A"]
[]
[]
[]
[]
["","","","","","2MXF40A2V1B","2MXF50A2V1B"]
["Abmessungen","Maßeinheit","","Höhe","mm","550","550"]
["","","","Breite","mm","765","765"]
["","","","Tiefe","mm","285","285"]
["Gewicht","Maßeinheit","","","kg","36","41"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","500","500"]
["","","Heizen","Sehr niedrig","U/min","320","500"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","-10","-10"]
["","","","Max.","°C TK","46","46"]
["","Heizen","Umgebung","Betriebsbereich-=-Heizen-=-Umgebung-=-Min.-=-°C FK","°C FK","-15","-15"]
["","","","Betriebsbereich-=-Heizen-=-Umgebung-=-Max.-=-°C FK","°C FK","18","18"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","46","48"]
["","Heizen","","Hoch","dB(A)","48","50"]
["Kältemittel","Typ","","","","R-32","R-32"]
["","Füllmenge","","","kg","0.88","1.15"]
["","Kältemittel-=-Füllmenge-=-tCO2-Äq.","","","tCO2-Äq.","0.60","0.78"]
["","GWP","","","","675","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","20 (1)","20 (1)"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 20 m)","0,02 (für Rohrleitungslängen über 20 m)"]
["","Niveauunterschied","IG - AG","Max.","m","15.0","15.0"]
["","","IG - IG","Max.","m","7.5","7.5"]
["","Gesamtleitungslänge","System","Ist","m","30","30"]
["Standardzubehör","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Screw bag","","","","1","1"]
["Stromversorgung","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["Spannungsversorgung","Spannung","","","V","220-230-240","220-230-240"]
["Hinweise","","","","","(1) - Für 1Raum","(1) - Für 1Raum"]
["","","","","","(2) - Siehe separate Zeichnung für den Betriebsbereich","(2) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten","(3) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","","(4) - Enthält fluorierte Treibhausgase","(4) - Enthält fluorierte Treibhausgase"]
["Standardzubehör","Reducer assembly","","","","","1"]