{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-A9"]
[]
[]
[]
[]
["","","","","","2MXM40A2V1B9","2MXM50A2V1B9","2MXM68A2V1B9"]
["Abmessungen","Maßeinheit","","Höhe","mm","552","552","734"]
["","","","Breite","mm","852","852","974"]
["","","","Tiefe","mm","350","350","408"]
["Gewicht","Maßeinheit","","","kg","36","41","60"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","-10","-10","-10"]
["","","","Max.","°C TK","46","46","46"]
["Schalldruckpegel","Kühlung","","Nom.","dB(A)","46","48","48"]
["","Heizen","","Nom.","dB(A)","48","50","48"]
["Kältemittel","Typ","","","","R-32","R-32","R-32"]
["","Füllmenge","","","kg","0.88","1.15","2"]
["","Kältemittel-=-Füllmenge-=-tCO2-Äq.","","","tCO2-Äq.","0.60","0.78","1.35"]
["","GWP","","","","675","675","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","20 (1)","20 (1)","25 (1)"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 20 m)","0,02 (für Rohrleitungslängen über 20 m)","0,02 (für Rohrleitungslängen über 30 m)"]
["","Niveauunterschied","IG - AG","Max.","m","15","15","15"]
["","","IG - IG","Max.","m","7.5","7.5","7.5"]
["","Gesamtleitungslänge","System","Ist","m","30","30","50"]
["Standardzubehör","Installationsanleitung","","","","1","1","1"]
["","Ablassstopfen","","","","1","1","1"]
["","Schraubensack","","","","1","1","1"]
["Energieeffizienzbereich","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Stromversorgung","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240"]
["Hinweise","","","","","(1) - Für 1Raum","(1) - Für 1Raum","(1) - Für 1Raum"]
["","","","","","(2) - Bei Kombination mit CVXM-A, FVXM-A- maximale Rohrleitungslänge 30m.","(2) - Bei Kombination mit CVXM-A, FVXM-A- maximale Rohrleitungslänge 30m.","(2) - Bei Kombination mit CVXM-A, FVXM-A- maximale Rohrleitungslänge 30m."]
["","","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich","(3) - Siehe separate Zeichnung für den Betriebsbereich","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten","(4) - Siehe separate Zeichnung für die elektrischen Daten","(4) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","","(5) - Enthält fluorierte Treibhausgase","(5) - Enthält fluorierte Treibhausgase","(5) - Enthält fluorierte Treibhausgase"]
["Standardzubehör","Reduzierstück","","","","","1","1"]
["","Kondensatkappe","","","","","","3"]