{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-N"]
[]
[]
[]
[]
["","","","","","2MXM40N2V1B","2MXM50N2V1B","2MXM68N2V1B"]
["Abmessungen","Maßeinheit","","Höhe","mm","550","550","734"]
["","","","Breite","mm","765","765","958"]
["","","","Tiefe","mm","285","285","340"]
["Gewicht","Maßeinheit","","","kg","36","41","60"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","500","500","420"]
["","","Heizen","Sehr niedrig","U/min","320","500","420"]
["Verdichter","Type","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","","","-10"]
["","","","Max.","°C TK","","","46"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","46","48"]
["","","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dBA","","","48"]
["","Heizen","","Hoch","dBA","48","50"]
["","","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dBA","","","48.0"]
["Kältemittel","Typ","","","","R-32","R-32","R-32"]
["","Füllmenge","","","kg","0.88","1.15","2"]
["","Füllmenge","","","tCO2Eq","0.60","0.78","1.35"]
["","GWP","","","","675","675","675.0"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","20","20","25"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 20 m)","0,02 (für Rohrleitungslängen über 20 m)","0,02 (für Rohrleitungslängen über 30 m)"]
["","Niveauunterschied","IG - AG","Max.","M","15.0","15.0","15.0"]
["","","IG - IG","Max.","M","7.5","7.5","7.5"]
["","Gesamtleitungslänge","System","Ist","M","30","30","50"]
["Standardzubehör","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Stromversorgung","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-230-240","220-230-240","220-240"]
["Hinweise","","","","","(1) - Für 1 Raum","(1) - Für 1 Raum","(1) - Für 1 Raum"]
["Standardzubehör","Reducer assembly","","","","","1","1"]
["","Drain cap","","","","","","3"]