{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B2","2MXS40H3V1B","2MXS40H2V1B","2MXS50H3V1B2","2MXS50H3V1B","2MXS50H2V1B"]
["Schalldruckpegel","Heizen","","Nom.","dB(A)","48","48","","50","50"]
["","Kühlung","","Nom.","dB(A)","47","47","","48","48"]
["Standardzubehör","Installationsanleitung","","","","1","1","","1","1"]
["","Schraubensack","","","","1","1","","1","1"]
["","Ablassstopfen","","","","1","1","","1","1"]
["Kältemittel","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","GWP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Charge","","","kg","1.20","1.20","","1.60","1.60"]
["","Typ","","","","R-410A","R-410A","","R-410A","R-410A"]
["Rohrleitungsanschlüsse","Niveauunterschied","IG - IG","Max.","m","7.5","7.5","","7.5","7.5"]
["","","IG - AG","Max.","m","15","15","","15","15"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 20 m)","0,02 (für Rohrleitungslängen über 20 m)","","0,02 (für Rohrleitungslängen über 20 m)","0,02 (für Rohrleitungslängen über 20 m)"]
["","Gesamtleitungslänge","System","Ist","m","30","30","","30","30"]
["Verdichter","Typ","","","","Vollhermetischer Schwingverdichter","Vollhermetischer Schwingverdichter","","Vollhermetischer Schwingverdichter","Vollhermetischer Schwingverdichter"]
["Abmessungen","Maßeinheit","","Breite","mm","765","765","","765","765"]
["","","","Tiefe","mm","285","285","","285","285"]
["","","","Höhe","mm","550","550","","550","550"]
["Gewicht","Maßeinheit","","","kg","38","38","","42","42"]
["Power supply","Phase","","","","1~","1~","","1~","1~"]
["","Frequenz","","","Hz","50","50","","50","50"]
["","Spannung","","","V","220-240","220-240","","220-240","220-240"]
["Hinweise","","","","","(1) - Enthält fluorierte Treibhausgase","(1) - Enthält fluorierte Treibhausgase","","(1) - Enthält fluorierte Treibhausgase","(1) - Enthält fluorierte Treibhausgase"]
["Abmessungen","Maßeinheit","","Höhe","mm","","","550","","","550"]
["","","","Breite","mm","","","765","","","765"]
["","","","Tiefe","mm","","","285","","","285"]
["Gewicht","Maßeinheit","","","kg","","","38","","","42"]
["Verdichter","Typ","","","","","","Vollhermetischer Swing-Verdichter","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","","","10","","","10"]
["","","","Max.","°C TK","","","46","","","46"]
["","Heizen","Umgebung","Min.","°C FK","","","-15","","","-15"]
["","","","Max.","°C FK","","","15.5","","","15.5"]
["Schalldruckpegel","Kühlung","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dB(A)","","","47","","","48"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dB(A)","","","48","","","50"]
["Kältemittel","Typ","","","","","","R-410A","","","R-410A"]
["","Füllmenge","","","kg","","","1.20","","","1.60"]
["","Füllmenge","","","tCO2Eq","","","2.5","","","3.3"]
["","GWP","","","","","","2087.5","","","2087.5"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","","","20","","","20"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","","","0,02 (für Rohrleitungslängen über 20 m)","","","0,02 (für Rohrleitungslängen über 20 m)"]
["","Niveauunterschied","IG - AG","Max.","m","","","15","","","15"]
["","","IG - IG","Max.","m","","","7.5","","","7.5"]
["","Gesamtleitungslänge","System","Ist","m","","","30","","","30"]
["Standardzubehör","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["Stromversorgung","Phase","","","","","","1~","","","1~"]
["","Frequenz","","","Hz","","","50","","","50"]
["Spannungsversorgung","Spannung","","","V","","","220-240","","","220-240"]
["Standardzubehör","Reduzierstück","","","","","","","1","1"]
["","Reducer assembly","","","","","","","","","1"]