{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXF-A9"]
[]
[]
[]
[]
["","","","","","3AMXF52A2V1B9"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","420"]
["","","Heizen","Sehr niedrig","U/min","420"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°CTK","-10"]
["","","","Max.","°CTK","46"]
["Schalldruckpegel","Kühlung","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dB(A)","46"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dB(A)","47.0"]
["Kältemittel","Füllmenge","","","kg","1.8"]
["","Füllmenge","","","tCO2Eq","1.22"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","25 (1)"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 30 m)"]
["","Niveauunterschied","IG - AG","Max.","m","15.0"]
["","","IG - IG","Max.","m","7.5"]
["","Gesamtleitungslänge","System","Ist","m","50"]
["Standardzubehör","Installation manual","","","","1"]
["","Drain cap","","","","3"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Hinweise","","","","","(1) - Für 1 Raum"]