{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Schalldruckpegel","Heizen","","Nom.","dBA","47"]
["","Kühlung","","Nom.","dBA","46"]
["Standardzubehör","Installationsanleitung","","","","1"]
["","Schraubensack","","","","1"]
["","Ablassstopfen","","","","1"]
["","Kondensatkappe (1)","","","","6"]
["","Kondensatkappe (2)","","","","3"]
["","F-Gase-Aufkleber abziehen","","","","1"]
["","Zusätzliches Kältemitteletikett","","","","1"]
["Kältemittel","Charge","","","TCO2-Äquivalent","1.2"]
["","GWP","","","","675"]
["","Füllmenge","","","kg","1.8"]
["","Typ","","","","R-32"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","420"]
["","","Heizen","Sehr niedrig","U/min","420"]
["Rohrleitungsanschlüsse","Niveauunterschied","IG - IG","Max.","M","7.5"]
["","","IG - AG","Max.","M","15"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 30 m)"]
["","Gesamtleitungslänge","System","Ist","M","50"]
["Verdichter","Typ","","","","Vollhermetischer Schwingverdichter"]
["Abmessungen","Maßeinheit","","Breite","mm","868"]
["","","","Tiefe","mm","320"]
["","","","Höhe","mm","734"]
["Gewicht","Maßeinheit","","","kg","57"]
["Power supply","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["","Spannung","","","V","220-240"]
["Hinweise","","","","","(1) - Enthält fluorierte Treibhausgase"]
["","","","","","(2) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten"]
["Ventilator","Luftstromvolumen","Kühlung","Sehr niedrig","m³/min","","24"]
["","","Heizen","Sehr niedrig","m³/min","","24"]
["","","","Sehr niedrig","cfm","","847"]
["","","Heizen","Sehr niedrig","cfm","","847"]
["Abmessungen","Maßeinheit","","Höhe","mm","","734"]
["","","","Breite","mm","","868"]
["","","","Tiefe","mm","","320"]
["Gewicht","Maßeinheit","","","kg","","57"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","","420"]
["","","Heizen","Sehr niedrig","U/min","","420"]
["Verdichter","Typ","","","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°CTK","","-10"]
["","","","Max.","°CTK","","46"]
["","Heizen","Umgebung","Min.","°C FK","","-15"]
["","","","Max.","°C FK","","18"]
["Schalldruckpegel","Kühlung","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dBA","","46"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dBA","","47"]
["Kältemittel","Typ","","","","","R-32"]
["","Füllmenge","","","kg","","1.80"]
["","Füllmenge","","","tCO2Eq","","1.2"]
["","GWP","","","","","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","","25"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","","0,02 (für Rohrleitungslängen über 30 m)"]
["","Niveauunterschied","IG - AG","Max.","M","","15"]
["","","IG - IG","Max.","M","","7.5"]
["","Gesamtleitungslänge","System","Ist","M","","50"]
["Standardzubehör","Installation manual","","","","","1"]
["","Drain plug","","","","","1"]
["","Screw bag","","","","","1"]
["Stromversorgung","Phase","","","","","1~"]
["","Frequenz","","","Hz","","50"]
["Spannungsversorgung","Spannung","","","V","","220-240"]