{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-A9"]
[]
[]
[]
[]
["","","","","","3MXM40A2V1B9","3MXM52A2V1B9","3MXM68A2V1B9"]
["Abmessungen","Maßeinheit","","Höhe","mm","734","734","734"]
["","","","Breite","mm","974","974","974"]
["","","","Tiefe","mm","408","408","408"]
["Gewicht","Maßeinheit","","","kg","57","57","62"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","-10","-10","-10"]
["","","","Max.","°C TK","46","46","46"]
["Schalldruckpegel","Kühlung","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dB(A)","46","46","48"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dB(A)","47","47","48"]
["Kältemittel","Typ","","","","R-32","R-32","R-32"]
["","Füllmenge","","","kg","1.8","1.8","2"]
["","Füllmenge","","","tCO2Eq","1.22","1.22","1.35"]
["","GWP","","","","675","675","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","25 (1)","25 (1)","25 (1)"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 30 m)","0,02 (für Rohrleitungslängen über 30 m)","0,02 (für Rohrleitungslängen über 30 m)"]
["","Niveauunterschied","IG - AG","Max.","m","15","15","15"]
["","","IG - IG","Max.","m","7.5","7.5","7.5"]
["","Gesamtleitungslänge","System","Ist","m","50 (2)","50 (2)","50"]
["Standardzubehör","Installation manual","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["","Reducer assembly","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Stromversorgung","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240"]
["Hinweise","","","","","(1) - Für 1 Raum","(1) - Für 1 Raum"]
["","","","","","(2) - Bei Kombination mit CVXM-A, FVXM-A – maximale Rohrleitungslänge 30 m.","(2) - Bei Kombination mit CVXM-A, FVXM-A – maximale Rohrleitungslänge 30 m."]
["","","","","","","","(1) - Für 1 Raum"]