{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXM-M"]
[]
[]
[]
[]
["","","","","","5MXM90M2V1B"]
["Ventilator","Luftstromvolumen","Kühlung","Sehr niedrig","m³/min","24.1"]
["","","Heizen","Sehr niedrig","m³/min","24.1"]
["","","","Sehr niedrig","cfm","851"]
["","","Heizen","Sehr niedrig","cfm","851"]
["Abmessungen","Maßeinheit","","Höhe","mm","734"]
["","","","Breite","mm","320"]
["","","","Tiefe","mm","868"]
["Gewicht","Maßeinheit","","","kg","68"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","-10"]
["","","","Max.","°C TK","46"]
["","Heizen","Umgebung","Min.","°C FK","-15"]
["","","","Max.","°C FK","18"]
["Schalldruckpegel","Kühlung","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dB(A)","52"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dB(A)","52"]
["Kältemittel","Typ","","","","R-32"]
["","Füllmenge","","","kg","2.4"]
["","Füllmenge","","","tCO2Eq","1.6"]
["","GWP","","","","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","25"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 30 m)"]
["","Niveauunterschied","IG - AG","Max.","m","15"]
["","","IG - IG","Max.","m","7.5"]
["","Gesamtleitungslänge","System","Ist","m","75"]
["Standardzubehör","Installation manual","","","","1"]
["","Drain cap","","","","9"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Stromversorgung","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["Spannungsversorgung","Spannung","","","V","220-240"]