{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":8,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXS-E"]
[]
[]
[]
[]
["","","","","","5MXS90E3V3B2","5MXS90E3V3B","5MXS90E7V3B"]
["Schalldruckpegel","Heizen","","Nom.","dBA","52","52"]
["","Kühlung","","Nom.","dBA","52","52"]
["Standardzubehör","Installationsanleitung","","","","1","1"]
["","Ablassstopfen","","","","1","1"]
["","Reduzierstück","","","","1","1"]
["Kältemittel","Charge","","","TCO2-Äquivalent","6.2","6.2"]
["","GWP","","","","2,087.5","2,087.5"]
["","Füllmenge","","","kg","2.99","2.99"]
["","Typ","","","","R-410A","R-410A"]
["Betriebsbereich","Kühlung","Umgebung","Max.","°C TK","46"]
["","","","Min.","°C TK","-10"]
["","Heizen","Umgebung","Max.","°C FK","18"]
["","","","Min.","°C FK","-15"]
["Rohrleitungsanschlüsse","Niveauunterschied","IG - IG","Max.","M","7.5"]
["","","IG - AG","Max.","M","15"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 30 m)"]
["","Gesamtleitungslänge","System","Ist","M","75"]
["Verdichter","Typ","","","","Vollhermetischer Schwingverdichter"]
["Abmessungen","Maßeinheit","","Breite","mm","900","900"]
["","","","Tiefe","mm","320","320"]
["","","","Höhe","mm","770","770"]
["Gewicht","Maßeinheit","","","kg","73","73"]
["Power supply","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["","Spannung","","","V","230","230"]
["Hinweise","","","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, äquivalente Leitungslänge: 7,5 m","(1) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, äquivalente Leitungslänge: 7,5 m"]
["","","","","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 7,5 m","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 7,5 m"]
["","","","","","(3) - Enthält fluorierte Treibhausgase","(3) - Enthält fluorierte Treibhausgase"]
["Rohrleitungsanschlüsse","Niveauunterschied","IG - IG","Max.","M","","7.5"]
["","","IG - AG","Max.","M","","15"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","","0,02 (für Rohrleitungslängen über 30 m)"]
["","Gesamtleitungslänge","System","Ist","M","","75"]
["Verdichter","Typ","","","","","Vollhermetischer Schwingverdichter"]
["Abmessungen","Maßeinheit","","Höhe","mm","","","770"]
["","","","Breite","mm","","","900"]
["","","","Tiefe","mm","","","320"]
["Gewicht","Maßeinheit","","","kg","","","73"]
["Verdichter","Typ","","","","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","","","-10"]
["","","","Max.","°C TK","","","46"]
["","Heizen","Umgebung","Min.","°C FK","","","-15"]
["","","","Max.","°C FK","","","15.5"]
["Schalldruckpegel","Kühlung","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dBA","","","52"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dBA","","","52"]
["Kältemittel","Typ","","","","","","R-410A"]
["","Füllmenge","","","kg","","","2.99"]
["","Füllmenge","","","tCO2Eq","","","6.2"]
["","GWP","","","","","","2087.5"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","","","25"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","","","0,02 (für Rohrleitungslängen über 30 m)"]
["","Niveauunterschied","IG - AG","Max.","M","","","15"]
["","","IG - IG","Max.","M","","","7.5"]
["","Gesamtleitungslänge","System","Ist","M","","","75"]
["Standardzubehör","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["Stromversorgung","Phase","","","","","","1~"]
["","Frequenz","","","Hz","","","50"]
["Spannungsversorgung","Spannung","","","V","","","230"]