{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":76,"n_cols":9,"rows_kept":76,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Standardzubehör","Installationsanleitung","","","","Installationsanleitung"]
["","Bedienungsanleitung","","","","Bedienungsanleitung"]
["","Schraube + Unterlegscheibe","","","","Schraube + Unterlegscheibe"]
["","Infrarotfernbedienung","","","","Infrarotfernbedienung"]
["","Abdeckungsverriegelung Gitter","","","","Abdeckungsverriegelung Gitter"]
["","Batterie","","","","Batterie"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","9.52"]
["","Gas","","AD","mm","15.88"]
["","Ableitung","","","","19.05"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.128"]
["","Heizen","","Nom.","kW","0.128"]
["Schallleistungspegel","Kühlung","","","dBA","64"]
["","Heizen","","","dBA","64"]
["Abmessungen","Gerät","","Breite","mm","600"]
["","","","Tiefe","mm","1,007"]
["","","","Höhe","mm","285"]
["Gehäuse","Material","","","","Galvanisiertes Stahlblech"]
["Gewicht","Maßeinheit","","","kg","35"]
["Ventilator","Externer statischer Druck","","Hoch","Pa","90"]
["","","","Nom.","Pa","77"]
["","","","Niedrig","Pa","64"]
["Power supply","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["","Bezeichnung","","","","V1"]
["","Spannung","","","V","220-240"]
["Leistungsaufnahme","Heizen","","Nom.","kW","","0.109"]
["","Kühlung","","Nom.","kW","","0.109"]
["Ventilator","Externer statischer Druck","","Hoch","Pa","","70","150","150"]
["","","","Niedrig","Pa","","45","111","92"]
["Gehäuse","Material","","","","","Galvanisiertes Stahlblech"]
["Abmessungen","Maßeinheit","","Höhe","mm","","378","378","378"]
["","","","Breite","mm","","541","1300","1500"]
["","","","Tiefe","mm","","1045","541","541"]
["Gewicht","Maßeinheit","","","kg","","44","50","56"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37","44"]
["","","","Niedrig","m³/min","","18.3","34.8","37.9"]
["","","Heizen","Hoch","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37.4","43.9"]
["","","","Niedrig","m³/min","","18.3","34.8","37.9"]
["","Externer statischer Druck","","Nom.","Pa","","57","128","122"]
["Schallleistungspegel","Kühlung","","","dBA","","60","72","73"]
["","Heizen","","","dBA","","60","72","73"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","","41","53","55"]
["","","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dBA","","38"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dBA","","36","50","50"]
["","Heizen","","Hoch","dBA","","41","53","55"]
["","","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dBA","","38"]
["","","","Niedrig","dBA","","36","50","50"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","9.52","9.52","9.52"]
["","Gas","","AD","mm","","15.88","15.9","15.9"]
["","Ableitung","","","","","19.05"]
["Standardzubehör","Installation manual","","","","","Installation manual"]
["","Wireless remote control","","","","","Wireless remote control"]
["","Cover lock grill","","","","","Cover lock grill"]
["","Battery","","","","","Battery"]
["","Screw+Washer","","","","","Screw+Washer"]
["","Operation manual","","","","","Operation manual"]
["Stromversorgung","Bezeichnung","","","","","V1"]
["","Phase","","","","","1~"]
["","Frequenz","","","Hz","","50"]
["Spannungsversorgung","Spannung","","","V","","220-240"]
["Kühlleistung","Gesamtleistung","","Nom.","kW","","","12.10","13.00"]
["Heizleistung","Gesamtleistung","","Nom.","kW","","","13.5","15.5"]
["Gehäuse","Farbe","","","","","","Verzinktes Stahlblech / ohne Farbbeschichtung","Verzinktes Stahlblech / ohne Farbbeschichtung"]
["Ventilator","Luftstromvolumen","Kühlen","Mittel","m³/min","","","37","44"]
["","","Heizen","Mittel","m³/min","","","37.4","43.9"]
["Schalldruckpegel","Kühlen","","Mittel","dBA","","","52","53"]
["","Heizen","","Mittel","dBA","","","52","53"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","","","ARCWLA","ARCWLA"]