{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":98,"n_cols":9,"rows_kept":98,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Schalldruckpegel","Heizen","","Hoch","dB(A)","","44","","47"]
["","","","Nom.","dB(A)","","41","","44"]
["","","","Flüsterbetrieb","dB(A)","","36","","41"]
["","","","Niedrig","dB(A)","","38","","43"]
["","Kühlung","","Flüsterbetrieb","dB(A)","","36","","41"]
["","","","Niedrig","dB(A)","","38","","43"]
["","","","Hoch","dB(A)","","44","","47"]
["","","","Nom.","dB(A)","","41","","44"]
["Standardzubehör","Installationsanleitung","","","","","Installationsanleitung","","Installationsanleitung"]
["","Bedienungsanleitung","","","","","Bedienungsanleitung","","Bedienungsanleitung"]
["","Schrauben","","","","","Schrauben","","Schrauben"]
["","Unterlegscheibe","","","","","Unterlegscheibe","","Unterlegscheibe"]
["","Infrarotfernbedienung","","","","","Infrarotfernbedienung","","Infrarotfernbedienung"]
["","Abdeckungsverriegelung Gitter","","","","","Abdeckungsverriegelung Gitter","","Abdeckungsverriegelung Gitter"]
["","Batterie","","","","","Batterie","","Batterie"]
["Control systems","Wired remote control","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","9.52","","9.52"]
["","Gas","","AD","mm","","15.88","","15.88"]
["","Ableitung","","","","","19.05","","19.05"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","","0.094","","0.137"]
["","Heizen","","Nom.","kW","","0.094","","0.137"]
["Schallleistungspegel","Kühlung","","","dB(A)","","56","","60"]
["","Heizen","","","dB(A)","","56","","60"]
["Abmessungen","Maßeinheit","","Breite","mm","","820","","820"]
["","","","Tiefe","mm","","820","","820"]
["","","","Höhe","mm","","300","","300"]
["Gehäuse","Material","","","","","Galvanisiertes Stahlblech","","Galvanisiertes Stahlblech"]
["Gewicht","Maßeinheit","","","kg","","39","","39"]
["Ventilator","Luftstromvolumen","Heizen","Hoch","m³/min","","29.2","","34.0"]
["","","","Niedrig","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","Kühlung","Niedrig","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","","Hoch","m³/min","","29.2","","34.0"]
["","","","Flüsterbetrieb","m³/min","","17.6","","22.1"]
["","","Kühlung","Flüsterbetrieb","m³/min","","17.6","","22.1"]
["Geräteblende","Gewicht","","","kg","","4","","4"]
["","Abmessungen","","Höhe","mm","","82","","82"]
["","","","Tiefe","mm","","990","","990"]
["","","","Breite","mm","","990","","990"]
["","Farbe","","","","","Weiß","","Weiß"]
["Power supply","Phase","","","","","1~","","1~"]
["","Bezeichnung","","","","","V1","","V1"]
["","Frequenz","","","Hz","","50","","50"]
["","Spannung","","","V","","220-240","","220-240"]
["Ventilator","Luftstromvolumen","Heizen","Flüsterbetrieb","m³/min","15","","22.1"]
["Leistungsaufnahme","Heizen","","Nom.","kW","0.067","","0.137"]
["","Kühlung","","Nom.","kW","0.067","","0.137"]
["Ventilator","Luftstromvolumen","Kühlung","Flüsterbetrieb","m³/min","15","","22.1"]
["Gehäuse","Material","","","","Galvanisiertes Stahlblech","","Galvanisiertes Stahlblech"]
["Abmessungen","Maßeinheit","","Höhe","mm","265","","300"]
["","","","Breite","mm","820","","820"]
["","","","Tiefe","mm","820","","820"]
["Gewicht","Maßeinheit","","","kg","31","","39"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Niedrig","m³/min","17.6","","26.3"]
["","","Heizen","Hoch","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Niedrig","m³/min","17.6","","26.3"]
["Schallleistungspegel","Kühlung","","","dB(A)","54","","60"]
["","Heizen","","","dB(A)","54","","60"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","41","","47"]
["","","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dB(A)","38","","44"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","35","","43"]
["","","","Flüsterbetrieb","dB(A)","32","","41"]
["","Heizen","","Hoch","dB(A)","41","","47"]
["","","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dB(A)","38","","44"]
["","","","Niedrig","dB(A)","35","","43"]
["","","","Flüsterbetrieb","dB(A)","32","","41"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","9.52","","9.52"]
["","Gas","","AD","mm","15.88","","15.88"]
["","Ableitung","","","","19.05","","19.05"]
["Geräteblende","Farbe","","","","Weiß"]
["","Abmessungen","","Höhe","mm","82","","82"]
["","","","Breite","mm","990","","990"]
["","","","Tiefe","mm","990","","990"]
["","Gewicht","","","kg","4","","4"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","ARCWLA","","ARCWLA"]
["","Verkabelte Fernbedienung","","","","ARCWB","","ARCWB"]
["Standardzubehör","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Stromversorgung","Bezeichnung","","","","V1"]
["","Phase","","","","1~","","1~"]
["","Frequenz","","","Hz","50","","50"]
["Spannungsversorgung","Spannung","","","V","220-240","","220-240"]