{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / ARXM-A9"]
[]
[]
[]
[]
["","","","","ADEA35A2VEB / ARXM35A5V1B9","ADEA50A2VEB / ARXM50A5V1B9"]
["Kühlleistung","Nom.","","kW","3.4","5"]
["Heizleistung","Nom.","","kW","4","5.5"]
["Nominale Effizienz","EER","","","3.76","3.27"]
["","COP","","","3.97","3.74"]
["","Jährlicher Energieverbrauch","","kWh","452","765"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","A"]
["","","Heizen","","A","A"]
["Raumkühlen","Energieeffizienzklasse","","","A+","A+"]
["","Leistung","Pdesign","kW","3.4","5"]
["","SEER","","","5.9","5.65"]
["","Jährlicher Energieverbrauch","","kWh/a","202","310"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","A+","A+"]
["","Leistung","Pdesign","kW","2.9","4.4"]
["","SCOP/A","","","4.07","4"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung Pdh bei -10°-=-kW","","kW","2.32","3.73"]
["","Jährlicher Energieverbrauch","","kWh/a","997","1538"]
["Energieeffizienzbereich","","","","A+++ ~ D","A+++ ~ D"]
["Hinweise","","","","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","(3) - Nennkühlleistungen basieren auf: Innentemp.: 27°CTK, 19°CFK; Außentemperatur: 35°CTK; äquivalente Länge Kältemittelleitung: 5m; Niveauunterschied: 0m.","(3) - Nennkühlleistungen basieren auf: Innentemp.: 27°CTK, 19°CFK; Außentemperatur: 35°CTK; äquivalente Länge Kältemittelleitung: 5m; Niveauunterschied: 0m."]
["","","","","(4) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5m; Niveauunterschied: 0 m.","(4) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5m; Niveauunterschied: 0 m."]