{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":11,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXC-D"]
[]
[]
[]
[]
["","","","","","ARXC20DV1B","ARXC25DV1B","ARXC35DV1B","ARXC50DV1B","ARXC60DV1B","ARXC71DV1B"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","","45","46","51","54","54"]
["Kältemittel","GWP","","","","","675.0","675.0","675.0","675.0","675.0"]
["","Füllmenge","","","kg","","0.550","0.750","1.00","1.10","1.15"]
["","Typ","","","","","R-32","R-32","R-32","R-32","R-32"]
["Betriebsbereich","Kühlung","Umgebung","Max.","°CTK","","46","46","46","46","46"]
["","","","Min.","°CTK","","10","10","-10","-10","-10"]
["","Heizen","Umgebung","Max.","°C FK","","18","18","18","18","18"]
["","","","Min.","°C FK","","-15","-15","-15","-15","-15"]
["Rohrleitungsanschlüsse","Niveauunterschied","IG - AG","Max.","m","","15.0","15.0","20.0","20.0","20.0"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","","0,017 (für Rohrleitungslängen über 7,5 m)","0,017 (für Rohrleitungslängen über 7,5 m)","0,017 (für Rohrleitungslängen über 7,5 m)","0,017 (für Rohrleitungslängen über 7,5 m)","0,017 (für Rohrleitungslängen über 7,5 m)"]
["Sound power level","Kühlung","","","dB(A)","","58","60","65","66","69"]
["Abmessungen","Maßeinheit","","Breite","mm","","658","658","845","845","930"]
["","","","Tiefe","mm","","273","273","300","300","350"]
["","","","Höhe","mm","","550","550","615","615","695"]
["Verdichter","Typ","","","","","Hermetischer Swing","Hermetischer Swing","Hermetischer Swing","Hermetischer Swing","Hermetischer Swing"]
["Gewicht","Maßeinheit","","","kg","","24.0","26.0","39.0","39.0","45.0"]
["Power supply","Phase","","","","","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","","50","50","50","50","50"]
["","Spannung","","","V","","220-240","220-240","220-240","220-240","220-240"]
["Schallleistungspegel","Kühlung","","","dB(A)","58"]
["Abmessungen","Maßeinheit","","Höhe","mm","550"]
["","","","Breite","mm","658"]
["","","","Tiefe","mm","273"]
["Gewicht","Maßeinheit","","","kg","24"]
["Verdichter","Typ","","","","Hermetischer Swing"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°CTK","10"]
["","","","Max.","°CTK","46"]
["","Heizen","Umgebung","Min.","°C FK","-15"]
["","","","Max.","°C FK","18"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","45"]
["Kältemittel","Typ","","","","R-32"]
["","Füllmenge","","","kg","0.55"]
["","Füllmenge","","","tCO2Eq","0.371"]
["","GWP","","","","675.0"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","20"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,017 (für Rohrleitungslängen über 7,5 m)"]
["","Niveauunterschied","IG - AG","Max.","m","15.0"]
["Stromversorgung","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["Spannungsversorgung","Spannung","","","V","220-240"]