{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":7,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXD-A"]
[]
[]
[]
[]
["","","","","","ARXD25A5V1B","ARXD35A5V1B"]
["Abmessungen","Maßeinheit","","Höhe","mm","550","550"]
["","","","Breite","mm","765","765"]
["","","","Tiefe","mm","285","285"]
["Gewicht","Maßeinheit","","","kg","32","32"]
["Verdichter","Typ","","","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°CTK","-10","-10"]
["","","","Max.","°CTK","50","50"]
["Schalldruckpegel","Kühlung","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dB(A)","","49"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dB(A)","","49"]
["Kältemittel","Typ","","","","R-32","R-32"]
["","Füllmenge","","","kg","0.76","0.76"]
["","Füllmenge","","","tCO2Eq","","0.52"]
["","GWP","","","","675.0","675.0"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","20","20"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","m","15.0","15.0"]
["Standardzubehör","Installation manual","","","","","1"]
["","Refrigerant charge label","","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","1"]
["","General safety precautions","","","","","1"]
["","Drain plug","","","","","1"]
["Stromversorgung","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter"]
["Schalldruckpegel","Kühlung","","Nom.","dB(A)","46"]
["","Heizen","","Nom.","dB(A)","47"]
["Kältemittel","Kältemittel-=-Füllmenge-=-tCO2-Äq.","","","tCO2-Äq.","0.52"]
["Standardzubehör","Installationsanleitung","","","","1"]
["","Etikett für Kältemittelfüllmenge","","","","1"]
["","Mehrsprachige Etiketten über fluorierte Treibhausgase","","","","1"]
["","Allgemeine Schutzmaßnahmen","","","","1"]
["","Ablassstopfen","","","","1"]
["Energieeffizienzbereich","","","","","A+++ ~ D"]
["Hinweise","","","","","(1) - Enthält fluorierte Treibhausgase"]
["","","","","","(2) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten"]