{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":7,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-A9"]
[]
[]
[]
[]
["","","","","","ARXM35A5V1B9","ARXM50A5V1B9"]
["Abmessungen","Maßeinheit","","Höhe","mm","610","734"]
["","","","Breite","mm","923","954"]
["","","","Tiefe","mm","367","401"]
["Gewicht","Maßeinheit","","","kg","36","49"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","600","500"]
["Verdichter","Typ","","","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°CTK","-10","-10"]
["","","","Max.","°CTK","50","50 (1), 46 (1)"]
["","Heizen","Umgebung","Min.","°C FK","-21","-21 (1), -15 (1)"]
["","","","Max.","°C FK","18","18"]
["Schalldruckpegel","Kühlung","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dB(A)","","48"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dB(A)","","49"]
["Kältemittel","Typ","","","","R-32","R-32"]
["","Füllmenge","","","kg","0.95","1.1"]
["","Füllmenge","","","tCO2Eq","0.65","0.75"]
["","GWP","","","","675","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","20","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","m","15","20"]
["Standardzubehör","ARXM50A5V1B9","","","","","1"]
["","Installation manual","","","","1","1"]
["","Drain joint","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","LOT10 Energy Label","","","","1","1"]
["","Drain cap","","","","3","1"]
["Stromversorgung","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240"]
["Hinweise","","","","","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","","(3) - Enthält fluorierte Treibhausgase","(3) - Enthält fluorierte Treibhausgase"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter"]
["Schalldruckpegel","Kühlung","","Nom.","dB(A)","47"]
["","Heizen","","Nom.","dB(A)","49"]
["Standardzubehör","ARXM35A5V1B9","","","","1"]