{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-M"]
[]
[]
[]
[]
["","","","","","ARXM25M2V1B","ARXM35M2V1B","ARXM50MV1B"]
["Abmessungen","Maßeinheit","","Höhe","mm","550","550","735"]
["","","","Breite","mm","765","765","825"]
["","","","Tiefe","mm","285","285","300"]
["Gewicht","Maßeinheit","","","kg","32","32","44"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","-10","-10","-10"]
["","","","Max.","°C TK","46","46","46"]
["","Heizen","Umgebung","Min.","°C FK","-15","-15","-15"]
["","","","Max.","°C FK","18","18","18"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","46","49","48"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","","","44"]
["","Heizen","","Hoch","dB(A)","47","49","49"]
["","","","Niedrig","dB(A)","","","45"]
["Kältemittel","Typ","","","","R-32","R-32","R-32"]
["","Füllmenge","","","kg","0.76","0.76","1.4"]
["","Füllmenge","","","tCO2Eq","0.5","0.5","0.9"]
["","GWP","","","","675","675","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","15","15","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","M","12","12","20"]
["Standardzubehör","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1"]
["Stromversorgung","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240"]