{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":7,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Schalldruckpegel","Heizen","","Nom.","dBA","","49.0"]
["","Kühlung","","Nom.","dBA","","49.0"]
["Standardzubehör","Ablassstopfen","","","","","1"]
["","Installationsanleitung","","","","","1"]
["","Etikett für Kältemittelfüllmenge","","","","","1"]
["","Mehrsprachige Etiketten über fluorierte Treibhausgase","","","","","1"]
["","Allgemeine Schutzmaßnahmen","","","","","1"]
["Kältemittel","Charge","","","TCO2-Äquivalent","","0.52"]
["","GWP","","","","","675"]
["","Füllmenge","","","kg","","0.76"]
["","Typ","","","","","R-32"]
["Betriebsbereich","Kühlung","Umgebung","Max.","°C TK","","50 (4), 46 (5)"]
["","","","Min.","°C TK","","-10"]
["Rohrleitungsanschlüsse","Niveauunterschied","IG - AG","Max.","M","","15"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","","0,02 (für Rohrleitungslängen über 10 m)"]
["Verdichter","Typ","","","","","Vollhermetischer Schwingverdichter"]
["Abmessungen","Maßeinheit","","Breite","mm","","840"]
["","","","Tiefe","mm","","350"]
["","","","Höhe","mm","","552"]
["Gewicht","Maßeinheit","","","kg","","32"]
["Power supply","Phase","","","","","1~"]
["","Frequenz","","","Hz","","50"]
["","Spannung","","","V","","220-240"]
["Hinweise","","","","","(1) - Nur realisierbar in Kombination mit ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Enthält fluorierte Treibhausgase"]
["","","","","","(2) - Nur realisierbar in Kombination mit ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","","","(4) - Nur realisierbar in Kombination mit ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Nur realisierbar in Kombination mit ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Abmessungen","Maßeinheit","","Höhe","mm","552"]
["","","","Breite","mm","840"]
["","","","Tiefe","mm","350"]
["Gewicht","Maßeinheit","","","kg","32"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","-10"]
["","","","Max.","°C TK","50 (4), 46 (5)"]
["Schalldruckpegel","Kühlung","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dBA","46.0"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dBA","47.0"]
["Kältemittel","Typ","","","","R-32"]
["","Füllmenge","","","kg","0.76"]
["","Füllmenge","","","tCO2Eq","0.52"]
["","GWP","","","","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","20"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","M","15"]
["Standardzubehör","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Stromversorgung","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["Spannungsversorgung","Spannung","","","V","220-240"]