{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXP-N9"]
[]
[]
[]
[]
["","","","","","ARXP20N5V1B9","ARXP25N5V1B9","ARXP35N5V1B9"]
["Abmessungen","Maßeinheit","","Höhe","mm","556","556","556"]
["","","","Breite","mm","740","740","740"]
["","","","Tiefe","mm","343","343","343"]
["Gewicht","Maßeinheit","","","kg","24","24","26"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C Trockenkugel","-10","-10","-10"]
["","","","Max.","°C Trockenkugel","48","48","48"]
["","Heizen","Umgebung","Min.","°C Feuchtkugel","-15","-15","-15"]
["","","","Max.","°C Feuchtkugel","18","18","18"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","46","46","48"]
["","Heizen","","Hoch","dB(A)","47","47","48"]
["Kältemittel","Typ","","","","R-32","R-32","R-32"]
["","Füllmenge","","","kg","0.55","0.55","0.70"]
["","Füllmenge","","","tCO2Eq","0.37","0.37","0.48"]
["","GWP","","","","675.0","675.0","675.0"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","20","20","20"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","m","12","12","12"]
["Standardzubehör","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["Stromversorgung","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240"]