{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L"]
[]
[]
[]
[]
["","","","","","ARXS25L2V1B","ARXS35L2V1B","ARXS50L2V1B","ARXS60L2V1B","ARXS71L2V1B"]
["Schalldruckpegel","Heizen","","Hoch","dB(A)","47","48"]
["","","","Nom.","dB(A)","","","","49","52"]
["","Kühlung","","Hoch","dB(A)","46","48"]
["","","","Nom.","dB(A)","","","","49","52"]
["Standardzubehör","Installationsanleitung","","","","1","1","","1","1"]
["","Ablassstopfen","","","","1","1","","1","1"]
["","Mehrsprachige Etiketten über fluorierte Treibhausgase","","","","1","","","1","1"]
["","Etikett für Kältemittelfüllmenge","","","","1","","","1","1"]
["Kältemittel","Charge","","","TCO2-Äquivalent","2.1","2.5"]
["","GWP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Füllmenge","","","kg","1.0","1.2","","1.50","1.70"]
["","Typ","","","","R-410A","R-410A","","R-410A","R-410A"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","780","780"]
["","","Heizen","Sehr niedrig","U/min","740","740"]
["Betriebsbereich","Kühlung","Umgebung","Max.","°C Trockenkugel","46","46","","46","46"]
["","","","Min.","°C Trockenkugel","10","10","","-10","-10"]
["","Heizen","Umgebung","Max.","°C Feuchtkugel","18","18","","18","18"]
["","","","Min.","°C Feuchtkugel","-15","-15","","-15","-15"]
["Rohrleitungsanschlüsse","Niveauunterschied","IG - AG","Max.","M","15","15","","20.0","20.0"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["Schallleistungspegel","Kühlung","","","dB(A)","","","","62","65"]
["","Heizen","","","dB(A)","","","","62","65"]
["Verdichter","Typ","","","","Vollhermetischer Schwingverdichter","Vollhermetischer Schwingverdichter","","Vollhermetischer Schwingverdichter","Vollhermetischer Schwingverdichter"]
["Abmessungen","Maßeinheit","","Breite","mm","765","765","","825","825"]
["","","","Tiefe","mm","285","285","","300","300"]
["","","","Höhe","mm","550","550","","735","735"]
["Gewicht","Maßeinheit","","","kg","34","34","","47","47"]
["Ventilator","Luftstromvolumen","Heizen","Sehr niedrig","cfm","904","904"]
["","","","Sehr niedrig","m³/min","25.6","25.6"]
["","","Kühlung","Sehr niedrig","m³/min","30.1","30.1"]
["","","","Sehr niedrig","cfm","1,063","1,063"]
["Power supply","Phase","","","","1~","1~","","1~","1~"]
["","Frequenz","","","Hz","50","50","","50","50"]
["","Spannung","","","V","220-240","220-240","","220-230-240","220-230-240"]
["Hinweise","","","","","","","","(1) - Enthält fluorierte Treibhausgase","(1) - Enthält fluorierte Treibhausgase"]
["","","","","","(1) - Bei Anschluss an einem Multi-Außengerät lesen Sie bitte die technischen Gerätedaten des anzuschließenden Multi-Außengeräts.","(1) - Bei Anschluss an einem Multi-Außengerät lesen Sie bitte die technischen Gerätedaten des anzuschließenden Multi-Außengeräts.","(1) - 220 V"]
["","","","","","(2) - 220 V","(2) - 220 V","(2) - 230 V"]
["","","","","","(3) - 230 V","(3) - 230 V","(3) - 240 V"]
["","","","","","(4) - 240 V","(4) - 240 V"]
["","","","","","(5) - Enthält fluorierte Treibhausgase","(5) - Enthält fluorierte Treibhausgase"]
["Ventilator","Luftstromvolumen","Kühlung","Sehr niedrig","m³/min","","","48.9"]
["","","Heizen","Sehr niedrig","m³/min","","","43.1"]
["","","","Sehr niedrig","cfm","","","1727"]
["","","Heizen","Sehr niedrig","cfm","","","1522"]
["Abmessungen","Maßeinheit","","Höhe","mm","","","735"]
["","","","Breite","mm","","","825"]
["","","","Tiefe","mm","","","300"]
["Gewicht","Maßeinheit","","","kg","","","47"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","","","670"]
["","","Heizen","Sehr niedrig","U/min","","","670"]
["Verdichter","Typ","","","","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C Trockenkugel","","","10"]
["","","","Max.","°C Trockenkugel","","","46"]
["","Heizen","Umgebung","Min.","°C Feuchtkugel","","","-15"]
["","","","Max.","°C Feuchtkugel","","","18"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","","","48"]
["","Heizen","","Hoch","dB(A)","","","48"]
["Kältemittel","Typ","","","","","","R-410A"]
["","Füllmenge","","","kg","","","1.7"]
["","Füllmenge","","","tCO2Eq","","","3.5"]
["","GWP","","","","","","2087.5"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","","","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","","","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","M","","","20"]
["Standardzubehör","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["Stromversorgung","Phase","","","","","","1~"]
["","Frequenz","","","Hz","","","50"]
["Spannungsversorgung","Spannung","","","V","","","220-240"]