{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Schalldruckpegel","Heizen","","Hoch","dBA","","48"]
["","","","Niedrig","dBA","","45"]
["Standardzubehör","1","","","","","550"]
["Kältemittel","Charge","","","kg","","2.5"]
["","Typ","","","","","1.2"]
["Ventilator","Luftstromvolumen","Kühlung","Sehr niedrig","m³/min","","30.1"]
["","","","Sehr niedrig","Cfm","","1,063"]
["Ventilatormotor","Drehzahl","Kühlen","Sehr niedrig","U/min","","740"]
["","","Heizen","Sehr niedrig","U/min","","-15"]
["Betriebsbereich","Heizen","Umgebung","Min.","°C Feuchtkugel","","20"]
["","","","Max.","°C Feuchtkugel","","10"]
["Schalldruckpegel","Kühlung","","Niedrig","dBA","","44"]
["","","","Hoch","dBA","","48"]
["Compressor","Typ","","","","","Vollhermetischer Schwingverdichter"]
["Abmessungen","Maßeinheit","","Breite","mm","","285"]
["","","","Tiefe","mm","","612"]
["","","","Höhe","mm","","765"]
["Gewicht","Maßeinheit","","","kg","","34"]
["Ventilator","Luftstromvolumen","Heizen","Sehr niedrig","Cfm","","904"]
["","","","Sehr niedrig","m³/min","","25.6"]
["Power supply","Phase","","","","","1~"]
["","Frequenz","","","Hz","","50"]
["","Spannung","","","V","","220-240"]
["Hinweise","","","","","(1) - 220 V","(1) - Enthält fluorierte Treibhausgase"]
["","","","","","(2) - 230 V","(2) - 220 V"]
["","","","","","(3) - 240 V","(3) - 230 V"]
["","","","","","","(4) - 240 V"]
["Ventilator","Luftstromvolumen","Kühlung","Sehr niedrig","m³/min","30.1"]
["","","Heizen","Sehr niedrig","m³/min","25.6"]
["","","","Sehr niedrig","Cfm","1063"]
["","","Heizen","Sehr niedrig","Cfm","904"]
["Abmessungen","Maßeinheit","","Höhe","mm","550"]
["","","","Breite","mm","765"]
["","","","Tiefe","mm","285"]
["Gewicht","Maßeinheit","","","kg","34"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","780"]
["","","Heizen","Sehr niedrig","U/min","740"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C Trockenkugel","10"]
["","","","Max.","°C Trockenkugel","46"]
["","Heizen","Umgebung","Min.","°C Feuchtkugel","-15"]
["","","","Max.","°C Feuchtkugel","18"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","46"]
["","Heizen","","Hoch","dBA","47"]
["","","","Niedrig","dBA","44"]
["Kältemittel","Typ","","","","R-410A"]
["","Füllmenge","","","kg","1.0"]
["","Füllmenge","","","tCO2Eq","2.1"]
["","GWP","","","","2087.5"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","20"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","M","15"]
["Standardzubehör","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["Stromversorgung","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["Spannungsversorgung","Spannung","","","V","220-240"]