{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":9,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARYN-L"]
[]
[]
[]
[]
["","","","","ARYN20LV1","ARYN25LV1","ARYN35LV1","ARYN50LV1","ARYN60LV1"]
["Schalldruckpegel","Heizen","Nom.","dB(A)","44","46","49","52","52"]
["","Kühlung","Nom.","dB(A)","44","46","49","52","52"]
["Kältemittel","Charge","","TCO2Eq","1.4","1.7","1.8","3","3.4"]
["","GWP","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","kg","0.65","0.80","0.85","1.45","1.65"]
["","Typ","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Verdichter","Typ","","","Rollkolbenverdichter","Rollkolbenverdichter","Rollkolbenverdichter","Rollkolbenverdichter","Rollkolbenverdichter"]
["Abmessungen","Maßeinheit","Breite","mm","600","700","700","855","855"]
["","","Tiefe","mm","245","250","250","328","328"]
["","","Höhe","mm","494","540","540","651","753"]
["Gewicht","Maßeinheit","","kg","25","29","31","47","50"]
["Power supply","Phase","","","1~","1~","1~","1~","1~"]
["","Frequenz","","Hz","50","50","50","50","50"]
["","Spannung","","V","220-240","220-240","220-240","220-240","220-240"]
["Hinweise","","","","(1) - Alle Geräte sind getestet und entsprechen ISO 5151 (Gerät ohne Kanal) oder ISO 13253 (Gerät mit Kanal).","(1) - Alle Geräte sind getestet und entsprechen ISO 5151 (Gerät ohne Kanal) oder ISO 13253 (Gerät mit Kanal).","(1) - Alle Geräte sind getestet und entsprechen ISO 5151 (Gerät ohne Kanal) oder ISO 13253 (Gerät mit Kanal).","(1) - Alle Geräte sind getestet und entsprechen ISO 5151 (Gerät ohne Kanal) oder ISO 13253 (Gerät mit Kanal).","(1) - Alle Geräte sind getestet und entsprechen ISO 5151 (Gerät ohne Kanal) oder ISO 13253 (Gerät mit Kanal)."]
["","","","","(2) - Enthält fluorierte Treibhausgase","(2) - Enthält fluorierte Treibhausgase","(2) - Enthält fluorierte Treibhausgase","(2) - Enthält fluorierte Treibhausgase","(2) - Enthält fluorierte Treibhausgase"]