{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-J3"]
[]
[]
[]
[]
["","","","","","ATX20J3V1B","ATX25J3V1B","ATX35J3V1B"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.03","0.03","0.030"]
["","Heizen","","Nom.","kW","0.04","0.04","0.040"]
["Gehäuse","Farbe","","","","Weiß","Weiß","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","198","198","198"]
["","","","Breite","mm","770","770","770"]
["","","","Tiefe","mm","283","283","283"]
["Gewicht","Maßeinheit","","","kg","7","7","7.00"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","9.1","9.2","9.3"]
["","","Kühlen","Mittel","m³/min","7.4","7.6","7.7"]
["","","","Niedrig","m³/min","5.9","6","6.1"]
["","","","Flüsterbetrieb","m³/min","4.7","4.8","4.9"]
["","","Heizen","Hoch","m³/min","9.4","9.7","10.1"]
["","","","Mittel","m³/min","7.8","8","8.4"]
["","","","Niedrig","m³/min","6.3","6.3","6.7"]
["","","","Flüsterbetrieb","m³/min","5.5","5.5","5.7"]
["Schallleistungspegel","Kühlung","","","dB(A)","55","55","58"]
["","Heizen","","","dB(A)","55","55","58"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","39","40","41"]
["","Kühlen","","Mittel","dB(A)","33","33","34"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","25","26","27"]
["","","","Flüsterbetrieb","dB(A)","22","22","23"]
["","Heizen","","Hoch","dB(A)","39","40","41"]
["","","","Mittel","dB(A)","34","34","35"]
["","","","Niedrig","dB(A)","28","28","29"]
["","","","Flüsterbetrieb","dB(A)","25","25","26"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35","6.35"]
["","Gas","","AD","mm","9.5","9.5","9.50"]
["","Ableitung","","","","18","18","18"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","ARC433A89","ARC433A89","ARC433A89"]
["Standardzubehör","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Stromversorgung","Bezeichnung","","","","V1","V1","V1"]
["","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240"]