{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":11,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-KV"]
[]
[]
[]
[]
["","","","","","ATX20K2V1B","ATX20K5V1B","ATX25K2V1B","ATX25K5V1B","ATX35K5V1B","ATX35K2V1B (Archived)"]
["Schalldruckpegel","Heizen","","Hoch","dB(A)","","","","","","43"]
["","","","Mittel","dB(A)","","","","","","35"]
["","","","Flüsterbetrieb","dB(A)","","","","","","26"]
["","","","Niedrig","dB(A)","","","","","","29"]
["","Kühlung","","Medium","dB(A)","","","","","","34"]
["","","","Flüsterbetrieb","dB(A)","","","","","","20"]
["","","","Niedrig","dB(A)","","","","","","27"]
["","","","Hoch","dB(A)","","","","","","43"]
["Standardzubehör","Installationsanleitung","","","","","","","","","1"]
["","Bedienungsanleitung","","","","","","","","","1"]
["","Infrarot-Fernbedienung","","","","","","","","","1"]
["","Trockenbatterien, Typ AA","","","","","","","","","2"]
["","Fernbedienungshalterung","","","","","","","","","1"]
["","Montageplatte","","","","","","","","","1"]
["","Fotokatalytischer Luftreinigungsfilter mit Titanapatit","","","","","","","","","2"]
["","Befestigungsschrauben für Hauptgerät","","","","","","","","","2"]
["Regelungssysteme","Wired remote control","","","","","","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","","","","","","ARC480A11"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","","","","","6.35"]
["","Gas","","AD","mm","","","","","","9.50"]
["","Ableitung","","","","","","","","","18"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","","","","","","0.024"]
["","Heizen","","Nom.","kW","","","","","","0.029"]
["Sound power level","Kühlung","","","dB(A)","","","","","","58"]
["","Heizen","","","dB(A)","","","","","","58"]
["Abmessungen","Maßeinheit","","Breite","mm","","","","","","770"]
["","","","Tiefe","mm","","","","","","225"]
["","","","Höhe","mm","","","","","","286"]
["Gehäuse","Farbe","","","","","","","","","Weiß"]
["Gewicht","Maßeinheit","","","kg","","","","","","9.0"]
["Power supply","Phase","","","","","","","","","1~"]
["","Frequenz","","","Hz","","","","","","50"]
["","Bezeichnung","","","","","","","","","V1"]
["","Spannung","","","V","","","","","","220-240"]
["Hinweise","","","","","","","","","","(1) - SL: Die flüsterleise Ventilatorstufe der Luftmengeneinstellung."]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.018","0.018","0.02","0.02","0.024"]
["","Heizen","","Nom.","kW","0.022","0.022","0.023","0.023","0.029"]
["Gehäuse","Farbe","","","","Weiß","Weiß","Weiß","Weiß","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","286","286","286","286","286"]
["","","","Breite","mm","770","770","770","770","770"]
["","","","Tiefe","mm","225","225","225","225","225"]
["Gewicht","Maßeinheit","","","kg","8.5","8.5","8.5","8.5","9"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","9.9","9.9","10.4","10.4","11.8"]
["","","Kühlen","Mittel","m³/min","7.8","7.8","8","8","8.2"]
["","","","Niedrig","m³/min","5.8","5.8","6.1","6.1","6.3"]
["","","","Flüsterbetrieb","m³/min","4.8","4.8","4.8","4.8","4.9"]
["","","Heizen","Hoch","m³/min","10.9","10.9","11.1","11.1","12.8"]
["","","","Mittel","m³/min","8.5","8.5","8.5","8.5","8.5"]
["","","","Niedrig","m³/min","6.4","6.4","6.7","6.7","6.9"]
["","","","Flüsterbetrieb","m³/min","5.2","5.2","5.2","5.2","5.2"]
["Schallleistungspegel","Kühlung","","","dB(A)","55","55","55","55","58"]
["","Heizen","","","dB(A)","55","55","55","55","58"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","39","39","40","40","43"]
["","Kühlen","","Mittel","dB(A)","33","33","33","33","34"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","25","25","26","26","27"]
["","","","Flüsterbetrieb","dB(A)","20","20","20","20","20"]
["","Heizen","","Hoch","dB(A)","39","39","40","40","43"]
["","","","Mittel","dB(A)","34","34","34","34","35"]
["","","","Niedrig","dB(A)","28","28","28","28","29"]
["","","","Flüsterbetrieb","dB(A)","23","23","23","23","26"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","AD","mm","9.5","9.5","9.5","9.5","9.5"]
["","Ableitung","","","","18","18","18","18","18"]
["Regelungssysteme","Infrared remote control","","","","ARC480A11","ARC480A11","","","ARC480A11"]
["Regelungssysteme","Verkabelte Fernbedienung","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standardzubehör","Installation manual","","","","1","1","1","1","1"]
["","AA dry-cell batteries","","","","2","","2"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["Stromversorgung","Bezeichnung","","","","V1","V1","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240","220-240","220-240"]
["Standardzubehör","AAA dry-cell batteries","","","","","2","","2","2"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","","","ARC480A11","ARC480A11"]
["Standardzubehör","Titanium apatite photocatalytic air purification filter","","","","","","2"]