{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXC-D"]
[]
[]
[]
[]
["","","","","","ATXC20DV1B","ATXC25DV1B","ATXC35DV1B","ATXC50DV1B","ATXC60DV1B","ATXC71DV1B"]
["Schalldruckpegel","Kühlung","","Medium","dB(A)","","33","34","39","42","42"]
["","","","Flüsterbetrieb","dB(A)","","21","22","30","31","31"]
["","","","Niedrig","dB(A)","","26","26","33","38","38"]
["","","","Hoch","dB(A)","","40","41","47","48","48"]
["Regelungssysteme","Infrared remote control","","","","","ARC486A2","ARC486A2","ARC486A2","ARC486A2","ARC486A2"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","AD","mm","","9.52","9.52","12.7","12.7","12.7"]
["","Ableitung","","","","","16.5","16.5","16.5","16.5","16.5"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","","0.775","1.06","1.57","1.92","2.41"]
["","Heizen","","Nom.","kW","","0.755","1.08","1.52","1.73","2.49"]
["Sound power level","Kühlung","","","dB(A)","","57","58","60","63","63"]
["Abmessungen","Maßeinheit","","Breite","mm","","770","770","770","990","990"]
["","","","Tiefe","mm","","234","234","234","273","273"]
["","","","Höhe","mm","","288","288","288","297","297"]
["Gehäuse","Material","","","","","Hochschlagzähes Polystyrol","Hochschlagzähes Polystyrol","Hochschlagzähes Polystyrol","Hochschlagzähes Polystyrol","Hochschlagzähes Polystyrol"]
["","Farbe","","","","","Weiß","Weiß","Weiß","Weiß","Weiß"]
["Gewicht","Maßeinheit","","","kg","","9.00","9.50","9.50","13.0","13.0"]
["Ventilator","Luftstromvolumen","Kühlung","Niedrig","m³/min","","6.1","6.4","8.1","12.5","12.5"]
["","","","Mittel","m³/min","","8.1","8.7","9.9","14.5","14.5"]
["","","","Hoch","m³/min","","10.8","11.1","12.5","20.4","20.4"]
["","","","Flüsterbetrieb","m³/min","","5.4","5.4","7.4","10.2","10.2"]
["Power supply","Phase","","","","","1~","1~","1~","1~","1~"]
["","Bezeichnung","","","","","V1","V1","V1","V1","V1"]
["","Frequenz","","","Hz","","50","50","50","50","50"]
["","Spannung","","","V","","220-240","220-240","220-240","220-240","220-240"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.6"]
["","Heizen","","Nom.","kW","0.67"]
["Gehäuse","Farbe","","","","Weiß"]
["","Material","","","","Hochschlagzähes Polystyrol"]
["Abmessungen","Maßeinheit","","Höhe","mm","288"]
["","","","Breite","mm","770"]
["","","","Tiefe","mm","234"]
["Gewicht","Maßeinheit","","","kg","9"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","10.8"]
["","","Kühlen","Mittel","m³/min","8.1"]
["","","","Niedrig","m³/min","6.1"]
["","","","Flüsterbetrieb","m³/min","5.4"]
["Schallleistungspegel","Kühlung","","","dB(A)","57"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","40"]
["","Kühlen","","Mittel","dB(A)","33"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","26"]
["","","","Flüsterbetrieb","dB(A)","21"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35"]
["","Gas","","AD","mm","9.52"]
["","Ableitung","","","","16.5"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","ARC486A2"]
["Stromversorgung","Bezeichnung","","","","V1"]
["","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["Spannungsversorgung","Spannung","","","V","220-240"]