{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":7,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXD-A"]
[]
[]
[]
[]
["","","","","","ATXD25A5V1B","ATXD35A5V1B"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","","0.032"]
["","Heizen","","Nom.","kW","","0.032"]
["Gehäuse","Farbe","","","","","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","","286"]
["","","","Breite","mm","","770"]
["","","","Tiefe","mm","","225"]
["Gewicht","Maßeinheit","","","kg","","9.00"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","","11.0"]
["","","","Mittel","m³/min","","8.5"]
["","","","Niedrig","m³/min","","6.8"]
["","","","Flüsterbetrieb","m³/min","","5.4"]
["","","Heizen","Hoch","m³/min","","11.5"]
["","","","Mittel","m³/min","","9.4"]
["","","","Niedrig","m³/min","","7.7"]
["","","","Flüsterbetrieb","m³/min","","6.3"]
["Schallleistungspegel","Kühlung","","","dBA","","58"]
["","Heizen","","","dBA","","58"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","","43"]
["","","","Mittel","dBA","","34"]
["","","","Niedrig","dBA","","27"]
["","","","Flüsterbetrieb","dBA","","20"]
["","Heizen","","Hoch","dBA","","40"]
["","","","Mittel","dBA","","35"]
["","","","Niedrig","dBA","","29"]
["","","","Flüsterbetrieb","dBA","","21"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","6"]
["","Gas","","AD","mm","","9.50"]
["","Ableitung","","","","","18"]
["Regelungssysteme","Infrared remote control","","","","","ARC480A78"]
["","Verkabelte Fernbedienung","","","","","BRC944B2, BRC073A1"]
["Standardzubehör","Installationsanleitung","","","","","1"]
["","Bedienungsanleitung","","","","","1"]
["","Infrarot-Fernbedienung","","","","","1"]
["","Trockenbatterien, Typ AAA","","","","","2"]
["","Fernbedienungshalterung","","","","","1"]
["","Montageplatte","","","","","1"]
["","Geruchsfilter mit Titanapatit","","","","","1"]
["","Silber-Partikelfilter","","","","","1"]
["","Befestigungsschrauben für Hauptgerät","","","","","2"]
["","Allgemeine Schutzmaßnahmen","","","","","1"]
["Power supply","Phase","","","","","1~"]
["","Frequenz","","","Hz","","50"]
["","Spannung","","","V","","220-240"]
["Hinweise","","","","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 5 m; Niveauunterschied: 0 m"]
["","","","","","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m (horizontal)"]
["","","","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten"]
["Schallleistungspegel","Heizen","","","dBA","55"]
["","Kühlung","","","dBA","55"]
["Abmessungen","Maßeinheit","","Höhe","mm","286"]
["","","","Breite","mm","770"]
["","","","Tiefe","mm","225"]
["Gewicht","Maßeinheit","","","kg","8.5"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","40"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dBA","26"]
["","Heizen","","Hoch","dBA","40"]
["","","","Niedrig","dBA","28"]
["Standardzubehör","Installation manual","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Stromversorgung","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["Spannungsversorgung","Spannung","","","V","220-240"]