{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":87,"n_cols":11,"rows_kept":87,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A"]
[]
[]
[]
[]
["","","","","","ATXF20A5V1B","ATXF25A5V1B","ATXF35A5V1B","ATXF50A2V1B","ATXF60A2V1B","ATXF71A2V1B"]
["Schalldruckpegel","Heizen","","Hoch","dB(A)","40","","","42","44","45"]
["","","","Mittel","dB(A)","34","","","38","40","41"]
["","","","Flüsterbetrieb","dB(A)","21","","","30","32","33"]
["","","","Niedrig","dB(A)","28","","","33","35","36"]
["","Kühlung","","Medium","dB(A)","33","","","39","41","42"]
["","","","Flüsterbetrieb","dB(A)","20","","","31","33","34"]
["","","","Niedrig","dB(A)","26","","","34","36","37"]
["","","","Hoch","dB(A)","40","","","43","45","46"]
["Standardzubehör","Installationsanleitung","","","","1","","","1","1","1"]
["","Bedienungsanleitung","","","","1","","","1","1","1"]
["","Infrarot-Fernbedienung","","","","1","","","1","1","1"]
["","Trockenbatterien, Typ AAA","","","","2","","","2","2","2"]
["","Fernbedienungshalterung","","","","1","","","1","1","1"]
["","Montageplatte","","","","1","","","1","1","1"]
["","Befestigungsschrauben für Hauptgerät","","","","2","","","2","2","2"]
["Regelungssysteme","Wired remote control","","","","BRC944B2, BRC073A1","","","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","","","ARC470A1","ARC470A1","ARC470A1"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","","","6.35","6.35","6.35"]
["","Gas","","AD","mm","9.50","","","12.7","12.7","12.7"]
["","Ableitung","","","","18","","","18","18","18"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.019","","","0.029","0.032","0.032"]
["","Heizen","","Nom.","kW","0.020","","","0.032","0.035","0.035"]
["Sound power level","Kühlung","","","dB(A)","55","","","59","60","62"]
["","Heizen","","","dB(A)","55","","","61","62","62"]
["Abmessungen","Maßeinheit","","Breite","mm","770","","","990","990","990"]
["","","","Tiefe","mm","225","","","263","263","263"]
["","","","Höhe","mm","286","","","295","295","295"]
["Gehäuse","Farbe","","","","Weiß","","","Weiß","Weiß","Weiß"]
["Gewicht","Maßeinheit","","","kg","8.50","","","13.5","13.5","13.5"]
["Ventilator","Luftstromvolumen","Heizen","Hoch","m³/min","10.3","","","17.3","17.9","17.9"]
["","","","Niedrig","m³/min","6.7","","","12.2","12.8","12.8"]
["","","","Mittel","m³/min","8.6","","","14.8","15.8","15.8"]
["","","","Flüsterbetrieb","m³/min","5.3","","","10.7","11.3","11.3"]
["","","Kühlung","Niedrig","m³/min","6.1","","","11.9","12.2","12.2"]
["","","","Mittel","m³/min","8.1","","","14.4","14.8","14.8"]
["","","","Hoch","m³/min","10.1","","","16.8","17.3","17.3"]
["","","","Flüsterbetrieb","m³/min","4.4","","","10.5","10.7","10.7"]
["Power supply","Phase","","","","1~","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","","","50","50","50"]
["","Bezeichnung","","","","","","","V1","V1","V1"]
["","Spannung","","","V","220-240","","","220-240","220-240","220-240"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","","0.019","0.032"]
["","Heizen","","Nom.","kW","","0.02","0.032"]
["Gehäuse","Farbe","","","","","Weiß","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","","286","286"]
["","","","Breite","mm","","770","770"]
["","","","Tiefe","mm","","225","225"]
["Gewicht","Maßeinheit","","","kg","","8.5","9"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","","10.1","11.5"]
["","","Kühlen","Mittel","m³/min","","8.1","8.3"]
["","","","Niedrig","m³/min","","6.1","6.3"]
["","","","Flüsterbetrieb","m³/min","","4.4","4.5"]
["","","Heizen","Hoch","m³/min","","10.3","11.5"]
["","","","Mittel","m³/min","","8.6","9"]
["","","","Niedrig","m³/min","","6.7","7"]
["","","","Flüsterbetrieb","m³/min","","5.3","5.3"]
["Schallleistungspegel","Kühlung","","","dB(A)","","55","58"]
["","Heizen","","","dB(A)","","55","58"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","","40","43"]
["","Kühlen","","Mittel","dB(A)","","33","34"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","","26","27"]
["","","","Flüsterbetrieb","dB(A)","","20","20"]
["","Heizen","","Hoch","dB(A)","","40","40"]
["","","","Mittel","dB(A)","","34","35"]
["","","","Niedrig","dB(A)","","28","29"]
["","","","Flüsterbetrieb","dB(A)","","21","21"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","6.35","6.35"]
["","Gas","","AD","mm","","9.5","9.5"]
["","Ableitung","","","","","18","18"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","","ARC470A1","ARC470A1"]
["","Verkabelte Fernbedienung","","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standardzubehör","Installation manual","","","","","1","1"]
["","AAA dry-cell batteries","","","","","2","2"]
["","Operation manual","","","","","1","1"]
["","Indoor unit fixing screws","","","","","2","2"]
["","Infrared remote control","","","","","1","1"]
["","Mounting plate","","","","","1","1"]
["","Remote control holder","","","","","1","1"]
["Stromversorgung","Phase","","","","","1~","1~"]
["","Frequenz","","","Hz","","50","50"]
["Spannungsversorgung","Spannung","","","V","","220-240","220-240"]