{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXL-JV"]
[]
[]
[]
[]
["","","","","ATXL25J2V1B","ATXL35J2V1B"]
["Schalldruckpegel","Heizen","Hoch","dB(A)","41","41"]
["","","Flüsterbetrieb","dB(A)","26","26"]
["","","Niedrig","dB(A)","29","29"]
["","Kühlung","Flüsterbetrieb","dB(A)","23","23"]
["","","Niedrig","dB(A)","27","27"]
["","","Hoch","dB(A)","41","41"]
["","","Nom.","dB(A)","35","35"]
["","Kühlung","Nom.","dB(A)","34","34"]
["Standardzubehör","Installationsanleitung","","","1","1"]
["","Bedienungsanleitung","","","1","1"]
["","Infrarot-Fernbedienung","","","1","1"]
["","Batterien","","","2","2"]
["","Fernbedienungshalterung","","","1","1"]
["","Montageplatte","","","1","1"]
["","Fotokatalytischer Luftreinigungsfilter mit Titanapatit","","","2","2"]
["","Befestigungsschrauben für Hauptgerät","","","2","2"]
["Regelungssysteme","Infrared remote control","","","ARC433A87","ARC433A87"]
["Rohrleitungsanschlüsse","Flüssigkeit","AD","mm","6.35","6.35"]
["","Gas","AD","mm","9.5","9.5"]
["","Ableitung","","","18","18"]
["Leistungsaufnahme","Kühlung","Nom.","kW","0.040 (2), 0.040 (3), 0.040 (4)","0.040 (2), 0.040 (3), 0.040 (4)"]
["","Heizen","Nom.","kW","0.040 (2), 0.040 (3), 0.040 (4)","0.040 (2), 0.040 (3), 0.040 (4)"]
["Schallleistungspegel","Kühlung","","dB(A)","57","57"]
["","Heizen","","dB(A)","57","57"]
["Abmessungen","Maßeinheit","Breite","mm","770","770"]
["","","Tiefe","mm","198","198"]
["","","Höhe","mm","283","283"]
["Gehäuse","Farbe","","","Weiß","Weiß"]
["Gewicht","Maßeinheit","","kg","8","8"]
["Power supply","Phase","","","1~","1~"]
["","Frequenz","","Hz","50","50"]
["","Bezeichnung","","","V1","V1"]
["","Spannung","","V","220-240","220-240"]
["Hinweise","","","","(1) - Bei Anschluss an einem Multi-Außengerät lesen Sie bitte die technischen Gerätedaten des anzuschließenden Multi-Außengeräts.","(1) - Bei Anschluss an einem Multi-Außengerät lesen Sie bitte die technischen Gerätedaten des anzuschließenden Multi-Außengeräts."]
["","","","","(2) - 220 V","(2) - 220 V"]
["","","","","(3) - 230 V","(3) - 230 V"]
["","","","","(4) - 240 V","(4) - 240 V"]