{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":9,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-N"]
[]
[]
[]
[]
["","","","","","ATXM20N2V1B","ATXM25N2V1B","ATXM35N2V1B","ATXM50N2V1B"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.03","0.03","0.034","0.03"]
["","Heizen","","Nom.","kW","0.025","0.026","0.026","0.032"]
["Gehäuse","Farbe","","","","Weiß","Weiß","Weiß","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","294","294","294","300"]
["","","","Breite","mm","811","811","811","1040"]
["","","","Tiefe","mm","272","272","272","295"]
["Gewicht","Maßeinheit","","","kg","10","10","10","14.5"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","11.1","11.1","12.3","16.1"]
["","","Kühlen","Mittel","m³/min","7.9","8.1","8.3","14.2"]
["","","","Niedrig","m³/min","6","6.2","6.4","11.6"]
["","","","Flüsterbetrieb","m³/min","4.4","4.4","4.6","8.1"]
["","","Heizen","Hoch","m³/min","10.8","10.8","10.8","17.1"]
["","","","Mittel","m³/min","8.7","8.7","9","14.6"]
["","","","Niedrig","m³/min","6.5","6.8","7.1","12.2"]
["","","","Flüsterbetrieb","m³/min","5.3","5.3","5.3","10.7"]
["Schallleistungspegel","Kühlung","","","dBA","58","58","58","58"]
["","Heizen","","","dBA","55","55","55","58"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","41","41","45","44"]
["","Kühlen","","Mittel","dBA","33","33","33","40"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dBA","25","25","29","36"]
["","","","Flüsterbetrieb","dBA","19","19","19","27"]
["","Heizen","","Hoch","dBA","39","39","39","43"]
["","","","Mittel","dBA","34","34","35","39"]
["","","","Niedrig","dBA","26","27","28","34"]
["","","","Flüsterbetrieb","dBA","20","20","20","31"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35","6.35","6.35"]
["","Gas","","AD","mm","9.5","9.5","9.5","12.7"]
["","Ableitung","","","","18","18","18","18"]
["Regelungssysteme","Infrared remote control","","","","ARC466A33","ARC466A33","ARC466A33","ARC466A33"]
["Regelungssysteme","Verkabelte Fernbedienung","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standardzubehör","Installation manual","","","","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","WLAN adapter kit","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","2"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Stromversorgung","Bezeichnung","","","","V1","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240","220-240"]