{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":95,"n_cols":13,"rows_kept":95,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R"]
[]
[]
[]
[]
["","","","","","ATXM20R2V1B §$ ATXM20R5V1B","ATXM20R2V1B (Archived)","ATXM20R5V1B (Archived)","ATXM25R2V1B (Archived)","ATXM25R5V1B (Archived)","ATXM35R2V1B (Archived)","ATXM35R5V1B (Archived)","ATXM50R2V1B (Archived)"]
["Schalldruckpegel","Heizen","","Hoch","dBA","39"]
["","","","Mittel","dBA","34"]
["","","","Flüsterbetrieb","dBA","20"]
["","","","Niedrig","dBA","26"]
["","Kühlung","","Medium","dBA","33"]
["","","","Flüsterbetrieb","dBA","19"]
["","","","Niedrig","dBA","25"]
["","","","Hoch","dBA","41"]
["Standardzubehör","Installationsanleitung","","","","1"]
["","Bedienungsanleitung","","","","1"]
["","Infrarotfernbedienung","","","","1"]
["","Trockenbatterien, Typ AAA","","","","2"]
["","Fernbedienungshalterung","","","","1"]
["","Montageplatte","","","","1"]
["","Geruchsfilter mit Titanapatit","","","","1"]
["","Befestigungsschrauben für Hauptgerät","","","","2"]
["","WLAN-Adapterbausatz","","","","1"]
["Regelungssysteme","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A67"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35"]
["","Gas","","AD","mm","9.50"]
["","Drain","","","","18"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.029"]
["","Heizen","","Nom.","kW","0.023"]
["Schallleistungspegel","Kühlung","","","dBA","58"]
["","Heizen","","","dBA","55"]
["Abmessungen","Maßeinheit","","Breite","mm","778"]
["","","","Tiefe","mm","272"]
["","","","Höhe","mm","295"]
["Gehäuse","Colour","","","","Weiß"]
["Gewicht","Maßeinheit","","","kg","10.0"]
["Ventilator","Luftstromvolumen","Heizen","Hoch","m³/min","9.3"]
["","","","Mittel","m³/min","8.2"]
["","","","Niedrig","m³/min","6.2"]
["","","","Flüsterbetrieb","m³/min","5.1"]
["","","Kühlung","Niedrig","m³/min","5.7"]
["","","","Mittel","m³/min","7.5"]
["","","","Hoch","m³/min","10.5"]
["","","","Flüsterbetrieb","m³/min","4.3"]
["Power supply","Phase","","","","1~"]
["","Bezeichnung","","","","V1"]
["","Frequenz","","","Hz","50"]
["","Spannung","","","V","220-240"]
["Hinweise","","","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m","(1) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m","(1) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m","(1) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m","(1) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m","(1) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m","(1) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m","(1) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m"]
["","","","","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m","(2) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","","0.029","0.029","0.029","0.029","0.03","0.03","0.03"]
["","Heizen","","Nom.","kW","","0.023","0.023","0.022","0.022","0.027","0.027","0.032"]
["Gehäuse","Farbe","","","","","Weiß","Weiß","Weiß","Weiß","Weiß","Weiß","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","","295","295","295","295","295","295","299"]
["","","","Breite","mm","","778","778","778","778","778","778","998"]
["","","","Tiefe","mm","","272","272","272","272","272","272","292"]
["Gewicht","Maßeinheit","","","kg","","10","10","10","10","10","10","14.5"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","","10.5","10.5","10.5","10.5","11.3","11.3","15.8"]
["","","Kühlen","Mittel","m³/min","","7.5","7.5","7.6","7.6","7.8","7.8","14"]
["","","","Niedrig","m³/min","","5.7","5.7","5.7","5.7","6","6","11.4"]
["","","","Flüsterbetrieb","m³/min","","4.3","4.3","4.1","4.1","4.2","4.2","8.3"]
["","","Heizen","Hoch","m³/min","","9.3","9.3","9.8","9.8","9.8","9.8","15.8"]
["","","","Mittel","m³/min","","8.2","8.2","8","8","8.5","8.5","14.2"]
["","","","Niedrig","m³/min","","6.2","6.2","6.3","6.3","6.5","6.5","12"]
["","","","Flüsterbetrieb","m³/min","","5.1","5.1","4.9","4.9","4.9","4.9","10.5"]
["Schallleistungspegel","Kühlung","","","dB(A)","","58","58","58","58","58","58","58"]
["","Heizen","","","dB(A)","","55","55","55","55","55","55","58"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","","41","41","41","41","45","45","44"]
["","Kühlen","","Schalldruckpegel-=-Kühlen-=-Mittel-=-dB(A)","dB(A)","","33","33","33","33","33","33","40"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","","25","25","25","25","25","25","36"]
["","","","Flüsterbetrieb","dB(A)","","19","19","19","19","19","19","27"]
["","Heizen","","Hoch","dB(A)","","39","39","39","39","39","39","43"]
["","","","Schalldruckpegel-=-Heizen-=-Mittel-=-dB(A)","dB(A)","","34","34","34","34","35","35","39"]
["","","","Niedrig","dB(A)","","26","26","27","27","28","28","34"]
["","","","Flüsterbetrieb","dB(A)","","20","20","20","20","20","20","31"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","AD","mm","","9.5","9.5","9.5","9.5","9.5","9.5","12.7"]
["","Ableitung","","","","","18","18","18","18","18","18","18"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67"]
["","Verkabelte Fernbedienung","","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standardzubehör","Installation manual","","","","","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","","2","2","2","2","2","2","2"]
["","WLAN adapter kit","","","","","1","1","1","1","1","1","1"]
["","Operation manual","","","","","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","1","1","1","1","1","1","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","1","1"]
["Stromversorgung","Bezeichnung","","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Phase","","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","","50","50","50","50","50","50","50"]
["Spannungsversorgung","Spannung","","","V","","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standardzubehör","Silver particle filter","","","","","","","","","","","1"]