{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":7,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-K3 / ARXP-K3"]
[]
[]
[]
[]
["","","","","ATXP20K3V1B / ARXP20K3V1B","ATXP25K3V1B / ARXP25K3V1B","ATXP35K3V1B / ARXP35K3V1B"]
["Kühlleistung","Nom.","","kW","2.00","2.50","3.50"]
["Nominale Effizienz","EER","","","3.98","3.79","3.45"]
["","COP","","","4.77","4.36","4.02"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","A","A"]
["","","Heizen","","A","A","A"]
["Heizleistung","Nom.","","kW","2.50","3.00","4.00"]
["Hinweise","","","","(1) - Kühlen: T2: Innentemp. 26,6 °C TK, 19,4 °C FK, Außentemp. 48 °C TK [Btu/h / W]","(1) - Kühlen: T2: Innentemp. 26,6 °C TK, 19,4 °C FK, Außentemp. 48 °C TK [Btu/h / W]","(1) - Kühlen: T2: Innentemp. 26,6 °C TK, 19,4 °C FK, Außentemp. 48 °C TK [Btu/h / W]"]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten","(3) - Siehe separate Zeichnung für die elektrischen Daten","(3) - Siehe separate Zeichnung für die elektrischen Daten"]