{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":8,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-N9"]
[]
[]
[]
[]
["","","","","","ATXP20N5V1B9","ATXP25N5V1B9","ATXP35N5V1B9"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.019","0.020","0.032"]
["","Heizen","","Nom.","kW","0.023","0.023","0.032"]
["Gehäuse","Farbe","","","","Weiß","Weiß","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","286","286","286"]
["","","","Breite","mm","770","770","770"]
["","","","Tiefe","mm","225","225","225"]
["Gewicht","Maßeinheit","","","kg","8.50","8.50","9.00"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","9.5","9.7","11.5"]
["","","","Mittel","m³/min","7.4","7.7","8.3"]
["","","","Niedrig","m³/min","5.6","5.8","6.3"]
["","","","Flüsterbetrieb","m³/min","4.2","4.2","4.5"]
["","","Heizen","Hoch","m³/min","10.4","10.4","11.5"]
["","","","Mittel","m³/min","8.1","8.1","9.0"]
["","","","Niedrig","m³/min","6.2","6.4","7.0"]
["","","","Flüsterbetrieb","m³/min","5.2","5.2","5.1"]
["Sound power level","Kühlung","","","dBA","55","55","58"]
["","Heizen","","","dBA","55","55","58"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","39","40","43"]
["","","","Medium","dBA","33","33","34"]
["","","","Niedrig","dBA","25","26","27"]
["","","","Flüsterbetrieb","dBA","19","19","20"]
["","Heizen","","Hoch","dBA","39","40","40"]
["","","","Mittel","dBA","34","34","35"]
["","","","Niedrig","dBA","28","28","29"]
["","","","Flüsterbetrieb","dBA","21","21","21"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6","6","6"]
["","Gas","","AD","mm","9.50","9.50","9.50"]
["","Ableitung","","","","18","18","18"]
["Regelungssysteme","Infrared remote control","","","","ARC480A78","ARC480A78","ARC480A78"]
["","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standardzubehör","Installationsanleitung","","","","1","1","1"]
["","Bedienungsanleitung","","","","1","1","1"]
["","Infrarot-Fernbedienung","","","","1","1","1"]
["","Trockenbatterien, Typ AAA","","","","2","2","2"]
["","Fernbedienungshalterung","","","","1","1","1"]
["","Montageplatte","","","","1","1","1"]
["","Geruchsfilter mit Titanapatit","","","","1","1","1"]
["","Silber-Partikelfilter","","","","1","1","1"]
["","Befestigungsschrauben für Hauptgerät","","","","2","2","2"]
["","Allgemeine Schutzmaßnahmen","","","","1","1","1"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["","Spannung","","","V","220-240","220-240","220-240"]
["Hinweise","","","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 5 m; Niveauunterschied: 0 m","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 5 m; Niveauunterschied: 0 m","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 5 m; Niveauunterschied: 0 m"]
["","","","","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m (horizontal)","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m (horizontal)","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m (horizontal)"]
["","","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten","(3) - Siehe separate Zeichnung für die elektrischen Daten","(3) - Siehe separate Zeichnung für die elektrischen Daten"]