{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":7,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXTP-K"]
[]
[]
[]
[]
["","","","","","ATXTP25K3V1B","ATXTP35K3V1B"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.03","0.03"]
["","Heizen","","Nom.","kW","0.035","0.035"]
["Gehäuse","Farbe","","","","Weiß","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","285","285"]
["","","","Breite","mm","770","770"]
["","","","Tiefe","mm","225","225"]
["Gewicht","Maßeinheit","","","kg","9","9"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","10.6","11.4"]
["","","Kühlen","Mittel","m³/min","7.7","8.2"]
["","","","Niedrig","m³/min","5.3","5.4"]
["","","","Flüsterbetrieb","m³/min","4.3","4.3"]
["","","Heizen","Hoch","m³/min","11.2","10.8"]
["","","","Mittel","m³/min","8","7.8"]
["","","","Niedrig","m³/min","5.8","5.8"]
["","","","Flüsterbetrieb","m³/min","4.9","4.9"]
["Schallleistungspegel","Kühlung","","","dB(A)","58","58"]
["","Heizen","","","dB(A)","58","58"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","43","43"]
["","Kühlen","","Mittel","dB(A)","35","35"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","26","26"]
["","","","Flüsterbetrieb","dB(A)","21","21"]
["","Heizen","","Hoch","dB(A)","43","43"]
["","","","Mittel","dB(A)","35","35"]
["","","","Niedrig","dB(A)","26","26"]
["","","","Flüsterbetrieb","dB(A)","21","21"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35"]
["","Gas","","AD","mm","9.5","9.5"]
["","Ableitung","","","","16 (Innendurchmesser des Anschlussschlauchs)","16 (Innendurchmesser des Anschlussschlauchs)"]
["Control systems","Infrared remote control","","","","ARC480A11","ARC480A11"]
["Regelungssysteme","Verkabelte Fernbedienung","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standardzubehör","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Stromversorgung","Bezeichnung","","","","V1","V1"]
["","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240"]