{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AZAS-MY1"]
[]
[]
[]
[]
["","","","","","AZAS100M7Y1B","AZAS125M7Y1B","AZAS140M7Y1B"]
["Abmessungen","Maßeinheit","","Höhe","mm","990","990","990"]
["","","","Breite","mm","940","940","940"]
["","","","Tiefe","mm","320","320","320"]
["Gewicht","Maßeinheit","","","kg","","70"]
["Compressor","Typ","","","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C Trockenkugel","-5","-5","-5"]
["","","","Max.","°C Trockenkugel","46","46","46"]
["","Heizen","Umgebung","Min.","°C Feuchtkugel","-15","-15","-15"]
["","","","Max.","°C Feuchtkugel","15.5","15.5","15.5"]
["Schallleistungspegel","Kühlung","","","dBA","70","71","73"]
["","Heizen","","","dBA","","71","73 (1)"]
["Schalldruckpegel","Kühlung","","Nom.","dBA","","53"]
["","Heizen","","Nom.","dBA","","57"]
["Kältemittel","Typ","","","","R-32","R-32","R-32"]
["","Füllmenge","","","kg","2.60","2.60","2.90"]
["Kältemittel","GWP","","","","","675"]
["Kältemittel","Füllmenge","","","tCO2Eq","1.76","1.76","1.96"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","9.52","9.52","9.52"]
["Rohrleitungsanschlüsse","Gas","","AD","mm","","15.9"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","30","30","30"]
["","","System","Äquivalent","M","50","50","50"]
["","","","Unbefüllt","M","30","30","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","Siehe Installationsanleitung","Siehe Installationsanleitung","Siehe Installationsanleitung"]
["","Niveauunterschied","IG - AG","Max.","M","30.0","30.0","30.0"]
["","","IG - IG","Max.","M","0.5","0.5","0.5"]
["Standardzubehör","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["Stromversorgung","Phase","","","","3~","3~","3~"]
["","Stromversorgung-=-Frequenz","","Frequenz","","50","50","50"]
["Spannungsversorgung","Spannungsversorgung-=-Spannung","","Spannung","","380-415","380-415","380-415"]
["Strom - 50 Hz","Strom - 50 Hz-=-Höchstamperezahl für Sicherung (MSiA)","","Strom - 50 Hz-=-Höchstamperezahl für Sicherung (MSiA)-=-A","","","16"]
["Hinweise","","","","","","(1) - Gemäß ENER Lot 21","(1) - Gemäß ENER Lot 21"]
["Gewicht","Maßeinheit","","","kg","70","","77"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","","Vollhermetischer Swing-Verdichter"]
["Schalldruckpegel","Kühlung","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dBA","53","","54"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dBA","57","","57"]
["Kältemittel","GWP","","","","675","","675"]
["Rohrleitungsanschlüsse","Gas","","AD","mm","15.9","","15.9"]
["Stromstärke&nbsp;– 50&nbsp;Hz","Stromstärke&nbsp;– 50&nbsp;Hz-=-Max. Amperezahl für Sicherung (MFA)-=-A","","","A","16","","16"]