{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BR00000676"]
[]
[]
[]
[]
["","","","","","BR00000676."]
["Typ","","","","","Luftreiniger"]
["Betrieb","","","","","Truhengerät mit Verkleidung"]
["Leistung","m³/min","","","","33.33"]
["Gehäuse","Farbe","","","","Lackierter verzinkter Stahl"]
["Abmessungen","Maßeinheit","","Höhe","mm","1628"]
["","","","Breite","mm","720"]
["","","","Tiefe","mm","770"]
["Gewicht","Maßeinheit","","","kg","150"]
["Geeignete Raumgröße","m²","","","","133"]
["Betriebsart Luftreinigung","Leistungsaufnahme","","H","kW","0.379"]
["Schalldruckpegel","Betriebsart Luftreinigung","","Hoch","dBA","55.9"]
["Ventilator","Luftstromvolumen","Betriebsart Luftreinigung","Turbo","m³/h","2300"]
["","","","Hoch","m³/h","2000"]
["Verfahren für Staubsammeln","","","","","RedPleat Carbon, 592 x 592 x 45 C, Abscheidegrad HEPA H14"]
["Verfahren für Bakterienfilterung","","","","","Astrocel III HEPA H14, A39A05C9S2R1"]
["Schutzvorrichtungen","Angabe","","01","","Sicherheitsschalter (Betrieb stoppt, wenn die Klappe an der Rückseite geöffnet wird)"]
["Standardzubehör","Prefilter selected","","","","1"]
["","HEPA filter selected","","","","1"]
["","Quick Start and Maintenance Guide","","","","1"]
["","Installation and Operation Manual available for download","","","","1"]
["Netzkabel","M","","","","3"]
["Stromversorgung","Phase","","","","1~"]
["","Frequenz","","","Hz","50/60"]
["Spannungsversorgung","Spannung","","","V","230"]
["Betriebsstrom","Betriebsart Luftreinigung","","Hoch","A","1.73"]