{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1E53A"]
[]
[]
[]
[]
["","","","","BRC1E53A7"]
["Gehäuse","Farbe","","","Reinweiß"]
["","Tastenabdeckung","","","Nein"]
["","Betriebs-LED","Farbe","","Grün"]
["Abmessungen","Maßeinheit","Höhe","mm","120"]
["","","Breite","mm","120"]
["","","Tiefe","mm","19"]
["","Versandpaket","Höhe","mm","55"]
["","","Breite","mm","160"]
["","","Tiefe","mm","150"]
["Gewicht","Maßeinheit","","kg","0.200"]
["","Versandpaket","","kg","0.415"]
["Verpackung","Material","","","Karton_"]
["","Gewicht","","kg","0.05"]
["LCD","Typ","","","Voller Punkt (160 x 255)"]
["","Abmessungen","Höhe","mm","43.2"]
["","","Breite","mm","68.85"]
["","Hintergrundlicht","Farbe","","Weiß"]
["Umgebungstemperatur","Betrieb","Min.","°C","-10"]
["","","Max.","°C","50"]
["","Lagerung","Min.","°C","-20"]
["","","Max.","°C","70"]
["","Relative Luftfeuchte <","","%","95"]
["Verdrahtungsanschlüsse","Kabellänge","max.","m","500"]
["Reserve für Stromausfall","","","","Ja (Die Uhr läuft für maximal 48 Stunden weiter)"]