{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1H81W"]
[]
[]
[]
[]
["","","","","BRC1H81W."]
["Verpackung","Material","","","Karton"]
["","Gewicht","","kg","0.0850"]
["Umgebungstemperatur","Relative Luftfeuchte <","","%","95"]
["Abmessungen","Versandpaket","Breite","mm","217"]
["","","Höhe","mm","50"]
["","","Tiefe","mm","161"]
["","Maßeinheit","Breite","mm","85"]
["","","Tiefe","mm","25"]
["","","Höhe","mm","85"]
["Gehäuse","Tastenabdeckung","","","Nein"]
["","Farbe","","","Weiß"]
["","Betriebs-LED","Farbe","","Blue status indicator"]
["LCD","Typ","","","100 x 150 dots"]
["","Hintergrundlicht","Farbe","","Weiß"]
["","Abmessungen","Breite","mm","28.0"]
["","","Höhe","mm","40.7"]
["Gewicht","Versandpaket","","kg","0.317"]
["","Maßeinheit","","kg","0.110"]
["Verdrahtungsanschlüsse","Kabellänge","max.","M","500"]