{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDS"]
[]
[]
[]
[]
["","","","","BRC1HHDASA","BRC1HHDAS (Archived)"]
["Gehäuse","Farbe","","","Silbern","Silbern"]
["","Tastenabdeckung","","","Nein","Nein"]
["","Betriebs-LED","Farbe","","Blaue Statusanzeige","Blaue Statusanzeige"]
["Abmessungen","Maßeinheit","Höhe","mm","85","85"]
["","","Breite","mm","85","85"]
["","","Tiefe","mm","25","25"]
["","Versandpaket","Höhe","mm","50","50"]
["","","Breite","mm","217","217"]
["","","Tiefe","mm","161","161"]
["Gewicht","Maßeinheit","","kg","0.110","0.110"]
["","Versandpaket","","kg","0.317","0.317"]
["Verpackung","Material","","","Karton","Karton"]
["","Gewicht","","kg","0.0850","0.0850"]
["LCD","Typ","","","100 x 150 Punkte","100 x 150 Punkte"]
["","Abmessungen","Höhe","mm","40.7","40.7"]
["","","Breite","mm","28.0","28.0"]
["","Hintergrundlicht","Farbe","","Weiß","Weiß"]
["Umgebungstemperatur","Betrieb","Min.","°C","-10","-10"]
["","","Max.","°C","50","50"]
["","Lagerung","Min.","°C","-20","-20"]
["","","Max.","°C","70","70"]
["","Umgebungstemperatur-=-Relative Luftfeuchte <-=-%","","%","95","95"]
["Regelungssysteme","Klasse der Temperaturregelung","","","VI","VI"]
["","Beitrag zur saisonalen Effizienz Raumheizen","","%","4.0","4.0"]
["Verdrahtungsanschlüsse","Kabellänge","max.","M","500","500"]