{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CKHWSU-BV3"]
[]
[]
[]
[]
["","","","","","CKHWSU230BJV3"]
["Abmessungen","Gerät","Höhe","Speicher","mm","1855"]
["","Maßeinheit","","Breite","mm","595"]
["","","","Tiefe","mm","634"]
["Gewicht","Gerät","","Leer","kg","115"]
["Trinkwassererwärmer","Wasservolumen","","","l","230"]
["","Material","","","","Edelstahl (EN 1.4521)"]
["Speicher","Maximale Wassertemperatur","","","°C","65.0"]
["Trinkwassererwärmer","Energieeffizienzklasse","","","","C"]
["Reserveheizung","Leistung","","","kW","1.5"]
["Hinweise","","","","","(1) - Basierend auf ∆T = 45 K"]
["","","","","","(2) - Warmwasserdurchfluss"]
["","","","","","(3) - 2-polig, 10 A, Kurve 230 V"]
["","","","","","(4) - Der oben erwähnte Netzanschluss der Hydrobox ist ausschließlich für den Reserveheizer vorgesehen. Der Schaltkasten und die Pumpe der Hydrobox werden mit dem Außengerät geliefert."]