{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-BB"]
[]
[]
[]
[]
["","","","","","CTXA15B2V1BB"]
["Schalldruckpegel","Heizen","","Hoch","dBA","39"]
["","","","Mittel","dBA","32"]
["","","","Flüsterbetrieb","dBA","21"]
["","","","Niedrig","dBA","25"]
["","Kühlung","","Medium","dBA","32"]
["","","","Flüsterbetrieb","dBA","21"]
["","","","Niedrig","dBA","25"]
["","","","Hoch","dBA","39"]
["Standardzubehör","Installationsanleitung","","","","1"]
["","Bedienungsanleitung","","","","1"]
["","Luftfilter","","","","2"]
["","Infrarot-Fernbedienung","","","","1"]
["","Montageplatte für Fernbedienung","","","","1"]
["","Schraubensack","","","","1"]
["","Schraubenabdeckung","","","","2"]
["","Trockenbatterien, Typ AAA","","","","2"]
["","Allgemeine Schutzmaßnahmen","","","","1"]
["Kältemittel","GWP","","","","675.0"]
["Regelungssysteme","Wired remote control","","","","BRC073"]
["","Infrared remote control","","","","ARC466A58"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35"]
["","Gas","","AD","mm","9.50"]
["","Ableitung","","","","18"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.020"]
["","Heizen","","Nom.","kW","0.020"]
["Sound power level","Kühlung","","","dBA","57"]
["Abmessungen","Maßeinheit","","Breite","mm","798"]
["","","","Tiefe","mm","189"]
["","","","Höhe","mm","295"]
["Gehäuse","Farbe","","","","Schwarz"]
["Gewicht","Maßeinheit","","","kg","11.5"]
["Ventilator","Luftstromvolumen","Heizen","Hoch","m³/min","10.9"]
["","","","Mittel","m³/min","8.7"]
["","","","Niedrig","m³/min","6.4"]
["","","","Flüsterbetrieb","m³/min","4.5"]
["","","Kühlung","Niedrig","m³/min","6.1"]
["","","","Mittel","m³/min","8.2"]
["","","","Hoch","m³/min","11.0"]
["","","","Flüsterbetrieb","m³/min","4.6"]
["Power supply","Phase","","","","1~"]
["","Bezeichnung","","","","V1"]
["","Frequenz","","","Hz","50"]
["","Spannung","","","V","220-240"]