{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXF-C"]
[]
[]
[]
[]
["","","","","","CTXF20C5V1B","CTXF25C5V1B","CTXF35C5V1B"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.017","0.019","0.032"]
["","Heizen","","Nom.","kW","0.02","0.02","0.032"]
["Gehäuse","Farbe","","","","Weiß","Weiß","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","286","286","286"]
["","","","Breite","mm","770","770","770"]
["","","","Tiefe","mm","225","225","225"]
["Gewicht","Maßeinheit","","","kg","8.5","8","9"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","9.8","10.1","11.5"]
["Ventilator","Luftstromvolumen","Kühlung","Mittel","m³/min","8","8","8"]
["Ventilator","Luftstromvolumen","Kühlung","Niedrig","m³/min","5.9","6.1","6.3"]
["","","","Flüsterbetrieb","m³/min","4.4","4.4","4.5"]
["","","Heizen","Hoch","m³/min","10.3","10.3","11.5"]
["Ventilator","Luftstromvolumen","Heizen","Mittel","m³/min","8.4","8.6","9"]
["Ventilator","Luftstromvolumen","Heizen","Niedrig","m³/min","6.5","6.7","7"]
["","","","Flüsterbetrieb","m³/min","5.3","5.3","5.3"]
["Schallleistungspegel","Kühlung","","","dB(A)","55","55","58"]
["","Heizen","","","dB(A)","55","55","58"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","39","40","43"]
["Schalldruckpegel","Kühlung","","Mittel","dB(A)","33","33","34"]
["Schalldruckpegel","Kühlung","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","25","26","27"]
["","","","Flüsterbetrieb","dB(A)","20","20","20"]
["","Heizen","","Hoch","dB(A)","39","40","40"]
["","","","Mittel","dB(A)","34","34","35"]
["","","","Niedrig","dB(A)","28","28","29"]
["","","","Flüsterbetrieb","dB(A)","21","21","21"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35","6.35"]
["Rohrleitungsanschlüsse","Gas","","AD","mm","9.5","9.5","9.5"]
["Rohrleitungsanschlüsse","Ableitung","","","","18","18","18"]
["Regelungssysteme","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1"]
["","Verkabelte Fernbedienung","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standardzubehör","Installation manual","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Batteries","","","","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Infrared remote control","","","","1","1","1"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Stromversorgung","Phase","","","","1~","1~","1~"]
["","Stromversorgung-=-Frequenz","","Frequenz","","50","50","50"]
["Spannungsversorgung","Spannungsversorgung-=-Spannung","","Spannung","","220-440","220-440","220-440"]