{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":8,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXF-F"]
[]
[]
[]
[]
["","","","","","CTXF20F5V1B","CTXF25F5V1B","CTXF35F5V1B"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.023","0.023","0.029"]
["","Heizen","","Nom.","kW","0.023","0.023","0.023"]
["Gehäuse","Farbe","","","","Weiß","Weiß","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","286","286","286"]
["","","","Breite","mm","770","770","770"]
["","","","Tiefe","mm","225","225","225"]
["Gewicht","Maßeinheit","","","kg","8.5","8.5","9"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","9.8","9.8","10.9"]
["","","Kühlen","Mittel","m³/min","8","8","7"]
["","","","Niedrig","m³/min","6","6","5.7"]
["","","","Flüsterbetrieb","m³/min","4.3","4.3","4.6"]
["","","Heizen","Hoch","m³/min","10.4","10.4","9.3"]
["","","","Mittel","m³/min","8.3","8.4","7.5"]
["","","","Niedrig","m³/min","6.2","6.4","6"]
["","","","Flüsterbetrieb","m³/min","5.3","5.3","5.2"]
["Schallleistungspegel","Kühlung","","","dB(A)","53","54","54"]
["","Heizen","","","dB(A)","55","55","56"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","39","40","56"]
["","Kühlen","","Mittel","dB(A)","33","33"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","25","26"]
["","","","Flüsterbetrieb","dB(A)","20","20"]
["","Heizen","","Hoch","dB(A)","39","40","40"]
["","","","Mittel","dB(A)","33","34","35"]
["","","","Niedrig","dB(A)","28","28","29"]
["","","","Flüsterbetrieb","dB(A)","21","21","21"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6","6","6"]
["","Gas","","AD","mm","9.5","9.5","9.5"]
["","Ableitung","","","","18","18","18"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","ARC480A93","ARC480A93","ARC480A93"]
["","Verkabelte Fernbedienung","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standardzubehör","Installation manual","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Infrared remote control","","","","1","1","1"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Stromversorgung","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-440","220-440","220-440"]
["Hinweise","","","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 5 m; Niveauunterschied: 0 m","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 5 m; Niveauunterschied: 0 m","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 5 m; Niveauunterschied: 0 m"]
["","","","","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m (horizontal)","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m (horizontal)","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m (horizontal)"]
["","","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten","(3) - Siehe separate Zeichnung für die elektrischen Daten","(3) - Siehe separate Zeichnung für die elektrischen Daten"]