{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":7,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-A"]
[]
[]
[]
[]
["","","","","","CTXM15A5V1B","CTXM15A2V1B"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.019","0.019"]
["","Heizen","","Nom.","kW","0.018","0.018"]
["Gehäuse","Farbe","","","","Weiß","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","298","298"]
["","","","Breite","mm","804","804"]
["","","","Tiefe","mm","252","252"]
["Gewicht","Maßeinheit","","","kg","11.5","11.5"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","11.9","11.9"]
["","","Kühlen","Mittel","m³/min","8.9","8.9"]
["","","","Niedrig","m³/min","6.3","6.3"]
["","","","Flüsterbetrieb","m³/min","4.9","4.9"]
["","","Heizen","Hoch","m³/min","11.4","11.4"]
["","","","Mittel","m³/min","9.2","9.2"]
["","","","Niedrig","m³/min","6.9","6.9"]
["","","","Flüsterbetrieb","m³/min","4.9","4.9"]
["Schallleistungspegel","Kühlung","","","dB(A)","54","54"]
["","Heizen","","","dB(A)","53","53"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","41","41"]
["","Kühlen","","Mittel","dB(A)","33","33"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","25","25"]
["","","","Flüsterbetrieb","dB(A)","19","19"]
["","Heizen","","Hoch","dB(A)","39","39"]
["","","","Mittel","dB(A)","34","34"]
["","","","Niedrig","dB(A)","26","26"]
["","","","Flüsterbetrieb","dB(A)","20","20"]
["Kältemittel","GWP","","","","675","675"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.4","6.4"]
["","Gas","","AD","mm","9.5","9.5"]
["","Ableitung","","","","16","16"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","ARC466A86","ARC466A86"]
["","Verkabelte Fernbedienung","","","","BRC073A1","BRC073A1"]
["Standardzubehör","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Installation plate","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Stromversorgung","Bezeichnung","","","","V1","V1"]
["","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240"]