{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R / 3MXM-A8"]
[]
[]
[]
[]
["","","","","CTXM15R5V1B / CTXM15R5V1B / CTXM15R5V1B / 3MXM40A2V1B8","CTXM15R2V1B / CTXM15R2V1B / CTXM15R2V1B / 3MXM40A2V1B8"]
["Kühlleistung","Nom.","","kW","4.00","4.00"]
["Heizleistung","Nom.","","kW","4.60","4.60"]
["Nominale Effizienz","EER","","","5.18","5.18"]
["","COP","","","5.17","5.17"]
["","Jährlicher Energieverbrauch","","kWh","386","386"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","A"]
["","","Heizen","","A","A"]
["Raumkühlen","Energieeffizienzklasse","","","A+++","A+++"]
["","Leistung","Pdesign","kW","4.00","4.00"]
["","SEER","","","8.55","8.55"]
["","Jährlicher Energieverbrauch","","kWh/a","164","164"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","A++","A++"]
["","Leistung","Pdesign","kW","4.90","4.90"]
["","SCOP/A","","","4.65","4.65"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung&nbsp;Pdh bei&nbsp;-10°-=-kW","","kW","4.00","4.00"]
["","Jährlicher Energieverbrauch","","kWh/a","1,475","1,475"]
["Hinweise","","","","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27°CTK, 19°CFK; Außentemperatur: 35°CTK; äquivalente Länge Kältemittelleitung: 5m; Niveauunterschied: 0m.","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27°CTK, 19°CFK; Außentemperatur: 35°CTK; äquivalente Länge Kältemittelleitung: 5m; Niveauunterschied: 0m."]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5m; Niveauunterschied: 0 m.","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5m; Niveauunterschied: 0 m."]
["","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten","(4) - Siehe separate Zeichnung für die elektrischen Daten"]