{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":7,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B (Archived)","CTXM15R5V1B (Archived)"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.029","0.029"]
["","Heizen","","Nom.","kW","0.023","0.023"]
["Gehäuse","Farbe","","","","Weiß","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","295","295"]
["","","","Breite","mm","778","778"]
["","","","Tiefe","mm","272","272"]
["Gewicht","Maßeinheit","","","kg","10","10"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","10.5","10.5"]
["","","Kühlen","Mittel","m³/min","7.5","7.5"]
["","","","Niedrig","m³/min","5.7","5.7"]
["","","","Flüsterbetrieb","m³/min","4.3","4.3"]
["","","Heizen","Hoch","m³/min","9.3","9.3"]
["","","","Mittel","m³/min","8.2","8.2"]
["","","","Niedrig","m³/min","6.2","6.2"]
["","","","Flüsterbetrieb","m³/min","5.1","5.1"]
["Schallleistungspegel","Kühlung","","","dB(A)","57","57"]
["","Heizen","","","dB(A)","54","54"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","41","41"]
["","Kühlen","","Schalldruckpegel-=-Kühlen-=-Mittel-=-dB(A)","dB(A)","33","33"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","25","25"]
["","","","Flüsterbetrieb","dB(A)","19","19"]
["","Heizen","","Hoch","dB(A)","39","39"]
["","","","Schalldruckpegel-=-Heizen-=-Mittel-=-dB(A)","dB(A)","34","34"]
["","","","Niedrig","dB(A)","26","26"]
["","","","Flüsterbetrieb","dB(A)","20","20"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35"]
["","Gas","","AD","mm","9.5","9.5"]
["","Ableitung","","","","18","18"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","ARC466A67","ARC466A67"]
["","Verkabelte Fernbedienung","","","","BRC073A1","BRC073A1"]
["Standardzubehör","Installationsanleitung","","","","1","1"]
["","Infrarotfernbedienung","","","","1","1"]
["","Trockenbatterien, Typ AAA","","","","2","2"]
["","WLAN-Adapterbausatz","","","","1","1"]
["","Bedienungsanleitung","","","","1","1"]
["","Geruchsfilter mit Titanapatit","","","","1","1"]
["","Befestigungsschrauben für Hauptgerät","","","","2","2"]
["","Montageplatte","","","","1","1"]
["","Fernbedienungshalterung","","","","1","1"]
["Energieeffizienzbereich","","","","","A+++ ~ D","A+++ ~ D"]
["Stromversorgung","Bezeichnung","","","","V1","V1"]
["","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240"]
["Hinweise","","","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m","(1) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m"]
["","","","","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m"]