{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Schalldruckpegel","Heizen","","Hoch","dBA","38","","41"]
["","","","Flüsterbetrieb","dBA","21","","21"]
["","","","Niedrig","dBA","28","","30"]
["","Kühlung","","Flüsterbetrieb","dBA","21","","21"]
["","","","Niedrig","dBA","25","","28"]
["","","","Hoch","dBA","37","","42"]
["","","","Nom.","dBA","33"]
["","Kühlung","","Nom.","dBA","31","","35"]
["Standardzubehör","Installationsanleitung","","","","1","","1"]
["","Bedienungsanleitung","","","","1","","1"]
["","Infrarotfernbedienung","","","","1","","1"]
["","Batterien","","","","2","","2"]
["","Fernbedienungshalterung","","","","1","","1"]
["","Montageplatte","","","","1","","1"]
["","Befestigungsschrauben für Hauptgerät","","","","2","","2"]
["","Fotokatalytischer Luftreinigungsfilter mit Titanapatit","","","","2","","2"]
["Regelungssysteme","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","","6.35"]
["","Gas","","AD","mm","9.5","","9.5"]
["","Ableitung","","","","18","","18"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.040","","0.040"]
["","Heizen","","Nom.","kW","0.040","","0.040"]
["Schallleistungspegel","Kühlung","","","dBA","55","","59"]
["","Heizen","","","dBA","56","","58"]
["Abmessungen","Gerät","","Breite","mm","780","","780"]
["","","","Tiefe","mm","215","","215"]
["","","","Höhe","mm","289","","289"]
["Gehäuse","Farbe","","","","Weiß","","Weiß"]
["Gewicht","Maßeinheit","","","kg","8","","8"]
["Ventilator","Luftstromvolumen","Heizen","Hoch","m³/min","","","10.1"]
["","","","Niedrig","m³/min","","","6.3"]
["","","","Flüsterbetrieb","m³/min","","","4.3"]
["","","Kühlen","Niedrig","m³/min","","","5.2"]
["","","","Hoch","m³/min","","","9.2"]
["","","","Flüsterbetrieb","m³/min","","","3.9"]
["","","","Nom.","m³/min","","","8.1"]
["","","Kühlen","Nom.","m³/min","","","7.2"]
["Power supply","Phase","","","","1~","","1~"]
["","Frequenz","","","Hz","50","","50"]
["","Bezeichnung","","","","V1","","V1"]
["","Spannung","","","V","220-240","","220-240"]
["Hinweise","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","","0.04","","0.040"]
["","Heizen","","Nom.","kW","","0.04","","0.040"]
["Gehäuse","Farbe","","","","","Weiß","","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","","289","","289"]
["","","","Breite","mm","","780","","780"]
["","","","Tiefe","mm","","215","","215"]
["Gewicht","Maßeinheit","","","kg","","8","","8.00"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","","7.9","","9.2"]
["","","Kühlen","Mittel","m³/min","","6.3","","7.2"]
["","","","Niedrig","m³/min","","4.7","","5.2"]
["","","","Flüsterbetrieb","m³/min","","3.9","","3.9"]
["","","Heizen","Hoch","m³/min","","9","","10.1"]
["","","","Mittel","m³/min","","7.5","","8.1"]
["","","","Niedrig","m³/min","","6","","6.3"]
["","","","Flüsterbetrieb","m³/min","","4.3","","4.3"]
["Schallleistungspegel","Kühlung","","","dBA","","55","","59"]
["","Heizen","","","dBA","","56","","58"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","","37","","42"]
["","Kühlen","","Mittel","dBA","","31","","35"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dBA","","25","","28"]
["","","","Flüsterbetrieb","dBA","","21","","21"]
["","Heizen","","Hoch","dBA","","38","","41"]
["","","","Mittel","dBA","","33","","36"]
["","","","Niedrig","dBA","","28","","30"]
["","","","Flüsterbetrieb","dBA","","21","","21"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","6.35","","6.35"]
["","Gas","","AD","mm","","9.5","","9.50"]
["","Ableitung","","","","","18","","18"]
["Regelungssysteme","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Standardzubehör","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Stromversorgung","Bezeichnung","","","","","V1","","V1"]
["","Phase","","","","","1~","","1~"]
["","Frequenz","","","Hz","","50","","50"]
["Spannungsversorgung","Spannung","","","V","","220-240","","220-240"]