{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":11,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2CND-A4A"]
[]
[]
[]
[]
["","","","","","D2CND024A4AB","D2CND024A4AA","D2CND028A4AA","D2CND028A4AB","D2CND035A4AA","D2CND035A4AB"]
["Gas","Verbrauch (G20)","","Min.","m³/h","0.31","0.31","0.511","0.511","0.511","0.511"]
["","","","Max.","m³/h","2.48","2.48","2.89","2.89","3.63","3.63"]
["","Verbrauch (G25)","","Min.","m³/h","0.36","0.36","0.59","0.59","0.59","0.59"]
["","","","Max.","m³/h","2.89","2.89","3.32","3.32","4.19","4.19"]
["","Verbrauch (G31)","","Min.","m³/h","0.12","0.12","0.2","0.2","0.2","0.2"]
["","","","Max.","m³/h","0.96","0.96","1.1","1.1","1.38","1.38"]
["","NOx-klasse","","","","6","6","6","6","6","6"]
["","NOx-Niveau (G20)","","","mg/kWh","22","22","36.3","36.3","35.5","35.5"]
["Zentralheizung","Heizaufnahme Qn (Netto-Brennwert)","Nom.","Min.","kW","2.9","2.9","4.8","4.8","4.8","4.8"]
["","","","Max.","kW","23.5","23.5","27","27","34","34"]
["","Heizaufnahme Qn (Brutto-Brennwert)","Nom.","Min.","kW","3.2","3.2","5.3","5.3","5.3","5.3"]
["","","","Max.","kW","26.1","26.1","30","30","37.8","37.8"]
["","Zentralheizung-=-Abgabe Pn bei 80/60&nbsp;°C","","Zentralheizung-=-Abgabe Pn bei 80/60&nbsp;°C-=-Min.-=-kW","kW","2.8","2.8","4.6","4.6","4.6","4.6"]
["","","","Zentralheizung-=-Abgabe Pn bei 80/60&nbsp;°C-=-Nom.-=-kW","kW","22.8","22.8","26.3","26.3","33.2","33.2"]
["","Zentralheizung-=-Abgabe Pnc bei 50/30&nbsp;°C","","Zentralheizung-=-Abgabe Pnc bei 50/30&nbsp;°C-=-Min.-=-kW","kW","3.1","3.1","5.2","5.2","5.2","5.2"]
["","","","Zentralheizung-=-Abgabe Pnc bei 50/30&nbsp;°C-=-Nom.-=-kW","kW","24","24.0","28.2","28.2","35","35"]
["","Zentralheizung-=-Abgabe bei 37/30&nbsp;°C","","Zentralheizung-=-Abgabe bei 37/30&nbsp;°C-=-Nom.-=-kW","kW","7.6","7.6","8.8","8.8","11.1","11.1"]
["","Wassertemperatur","","Max.","°C","100","100","100","100","100","100"]
["","Effizienz","","Netto-Brennwert","%","97.9","97.9"]
["","","","Brutto-Brennwert","%","87.3","87.3"]
["Trinkwassererwärmung","Heizaufnahme (Netto-Brennwert) Qnw","Nom.","Min.","kW","2.9","2.9","4.8","4.8","4.8","4.8"]
["","","","Max.","kW","23.5","23.5","29.5","29.5","34","34"]
["","Heizaufnahme (Brutto-Brennwert) Qnw","Nom.","Min.","kW","3.2","3.2","5.3","5.3","5.3","5.3"]
["","","","Max.","kW","26.1","26.1","32.7","32.7","37.7","37.7"]
["","Temperatur","","Max.","°C","60","60","60","60","60","60"]
["Wärmeverluste","Standby-Kessel Ps","","","kW","0.057","0.057","0.0650","0.065","0.0650","0.065"]
["Zufuhrluft","Anschluss","","","mm","100","100","100","100","100","100"]
["","Konzentrisch","","","","Ja","Ja","Ja","Ja","Ja","Ja"]
["Rauchgas","Temperatur","","Max.","°C","90","90","76.4","76.4","81.7","81.7"]
["","Anschluss","","","mm","60","60","60","60","60","60"]
["","Massendurchfluss (G20)","","Max.","kg/h","38.7","38.7","44.5","55.7","55.7","55.7"]
["","Massendurchfluss (G31)","","Max.","kg/h","36","36.0","43.3","43.3","54.7","54.7"]
["Gehäuse","Farbe","","","","Titan-Weiß (RAL 9003)","Titan-Weiß (RAL 9003)","Titan-Weiß (RAL 9003)","Titan-Weiß (RAL 9003)","Titan-Weiß (RAL 9003)","Titan-Weiß (RAL 9003)"]
["","Material","","","","Blech","Blech","Pulverlackiertes, verzinktes Stahlblech","Pulverlackiertes, verzinktes Stahlblech","Pulverlackiertes, verzinktes Stahlblech","Pulverlackiertes, verzinktes Stahlblech"]
["Abmessungen","Gerät","Höhe","Gehäuse","mm","590","590","690","690","690","690"]
["","Maßeinheit","","Breite","mm","400","400","440","440","440","440"]
["","","","Tiefe","mm","256","256","295","295","295","295"]
["Gewicht","Gerät","","Leer","kg","27","27","37","37","37","37"]
["","","","Voll","kg","27","27","39","","39"]
["","Kessel","","Leer","kg","27","27.0"]
["Trinkwassererwärmung","Allgemein","","Deklariertes Lastprofil","","XL","XL","XL","XL","XL","XL"]
["","","","Energieeffizienzklasse Wasserheizung","","A","A","A","A","A","A"]
["Raumheizen","Allgemein","","Saisonale Effizienzklasse Raumheizen","","A","A","A","A","A","A"]
["Rauchgas","Massendurchfluss (G25)","","Max.","kg/h","","","39.3","39.3","49.6","49.6"]