{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":8,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2CND-A5A"]
[]
[]
[]
[]
["","","","","","D2C18ND024A5AA","D2C20ND028A5AA","D2C24ND035A5AA"]
["Gas","Verbrauch (G20)","","Min.","m³/h","0.31","0.51","0.51"]
["","","","Max.","m³/h","1.80","2.04","2.45"]
["","Verbrauch (G25)","","Min.","m³/h","0.36","0.59","0.59"]
["","","","Max.","m³/h","2.09","2.35","2.85"]
["","Verbrauch (G31)","","Min.","m³/h","0.12","0.20","0.20"]
["","","","Max.","m³/h","0.69","0.98","1.19"]
["","NOx-klasse","","","","6","6","6"]
["","NOx-Niveau (G20)","","","mg/kWh","18","31","32"]
["Zentralheizung","Heizaufnahme Qn (Netto-Brennwert)","Nom.","Min.","kW","2.9","4.8","4.8"]
["","","","Max.","kW","16.9","19.2","23.5"]
["","Heizaufnahme Qn (Brutto-Brennwert)","Nom.","Min.","kW","3.2","5.3","5.3"]
["","","","Max.","kW","18.8","21.3","26.1"]
["","Zentralheizung-=-Abgabe Pn bei 80/60&nbsp;°C","","Zentralheizung-=-Abgabe Pn bei 80/60&nbsp;°C-=-Min.-=-kW","kW","2.8","4.6","4.6"]
["","","","Zentralheizung-=-Abgabe Pn bei 80/60&nbsp;°C-=-Nom.-=-kW","kW","16.4","18.8","22.9"]
["","Zentralheizung-=-Abgabe Pnc bei 50/30&nbsp;°C","","Zentralheizung-=-Abgabe Pnc bei 50/30&nbsp;°C-=-Min.-=-kW","kW","3.1","5.2","5.2"]
["","","","Zentralheizung-=-Abgabe Pnc bei 50/30&nbsp;°C-=-Nom.-=-kW","kW","18.0","20.0","24.0"]
["","Zentralheizung-=-Abgabe bei 37/30&nbsp;°C","","Zentralheizung-=-Abgabe bei 37/30&nbsp;°C-=-Nom.-=-kW","kW","5.5","6.3","7.7"]
["","Wassertemperatur","","Max.","°C","100","100","100"]
["Trinkwassererwärmung","Heizaufnahme (Netto-Brennwert) Qnw","Nom.","Min.","kW","2.9","4.8","4.8"]
["","","","Max.","kW","25.3","29.5","34.0"]
["","Heizaufnahme (Brutto-Brennwert) Qnw","Nom.","Min.","kW","3.2","5.3","5.3"]
["","","","Max.","kW","27.7","32.7","37.7"]
["","Komfortklassen (EN13203)","","","","***","***","***"]
["","Temperatur","","Max.","°C","70","70","70"]
["Zufuhrluft","Anschluss","","","mm","100","100","100"]
["","Konzentrisch","","","","Ja","Ja","Ja"]
["Rauchgas","Temperatur","","Max.","°C","77","76","82"]
["","Anschluss","","","mm","60","60","60"]
["","Massendurchfluss (G20)","","Max.","kg/h","38.7","44.5","55.7"]
["","Massendurchfluss (G31)","","Max.","kg/h","36.0","43.3","54.8"]
["Gehäuse","Farbe","","","","Titan-Weiß (RAL 9003)","Titan-Weiß (RAL 9003)","Titan-Weiß (RAL 9003)"]
["","Material","","","","Pulverlackiertes, verzinktes Stahlblech","Pulverlackiertes, verzinktes Stahlblech","Pulverlackiertes, verzinktes Stahlblech"]
["Abmessungen","Gerät","Höhe","Gehäuse","mm","590","695","695"]
["","Maßeinheit","","Breite","mm","400","440","440"]
["","","","Tiefe","mm","256","295","295"]
["Gewicht","Gerät","","Leer","kg","27","37","37"]
["Trinkwassererwärmung","Allgemein","","Deklariertes Lastprofil","","XL","XL","XL"]
["","","","Energieeffizienzklasse Wasserheizung","","A","A","A"]
["Raumheizen","Allgemein","","Saisonale Effizienzklasse Raumheizen","","A","A","A"]