{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2HND-A5A"]
[]
[]
[]
[]
["","","","","","D2HND012A5AA","D2HND018A5AA"]
["Gas","Verbrauch (G20)","","Min.","m³/h","0.31","0.31"]
["","","","Max.","m³/h","1.18","1.80"]
["","Verbrauch (G25)","","Min.","m³/h","0.36","0.36"]
["","","","Max.","m³/h","1.38","2.09"]
["","Verbrauch (G31)","","Min.","m³/h","0.12","0.12"]
["","","","Max.","m³/h","0.46","0.69"]
["","NOx-klasse","","","","6","6"]
["","NOx-Niveau (G20)","","","mg/kWh","10","18"]
["Zentralheizung","Heizaufnahme Qn (Netto-Brennwert)","Nom.","Min.","kW","2.9","2.9"]
["","","","Max.","kW","11.1","16.9"]
["","Heizaufnahme Qn (Brutto-Brennwert)","Nom.","Min.","kW","3.2","3.2"]
["","","","Max.","kW","12.3","18.8"]
["","Abgabe Pn bei 80/60 °C","","Min.","kW","2.8","2.8"]
["","","","Nom.","kW","10.8","16.4"]
["","Abgabe Pnc bei 50/30 °C","","Min.","kW","3.1","3.1"]
["","","","Nom.","kW","12.0","18.0"]
["","Abgabe bei 37/30 °C","","Nom.","kW","3.6","5.5"]
["","Wassertemperatur","","Max.","°C","100","100"]
["Raumheizen","Allgemein","","Saisonale Effizienzklasse Raumheizen","","A","A"]
["Zufuhrluft","Konzentrisch","","","","Ja","Ja"]
["Rauchgas","Temperatur","","Max.","°C","60","68"]
["","Massendurchfluss (G20)","","Max.","kg/h","18.4","28.0"]
["","Massendurchfluss (G31)","","Max.","kg/h","17.2","26.0"]
["Gehäuse","Farbe","","","","Titan-Weiß (RAL 9003)","Titan-Weiß (RAL 9003)"]
["","Material","","","","Pulverlackiertes, verzinktes Stahlblech","Pulverlackiertes, verzinktes Stahlblech"]
["Abmessungen","Maßeinheit","Höhe","Gehäuse","mm","590","590"]